--
-- Accedian Enterprise Specific MIB
--
-- Copyright (c) 2005-2016, Accedian Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--


ACD-CFM-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Integer32, Unsigned32, Counter32, Counter64, Gauge32
        FROM SNMPv2-SMI
    TruthValue, DateAndTime, RowStatus, MacAddress, TEXTUAL-CONVENTION, DisplayString
        FROM SNMPv2-TC
    VlanIdOrNone     FROM Q-BRIDGE-MIB  -- [RFC4363]

    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF

    acdMibs
        FROM ACCEDIAN-SMI;

acdCfm MODULE-IDENTITY

    LAST-UPDATED "201609230100Z"
    ORGANIZATION "Accedian Networks, Inc."
    CONTACT-INFO
            "Accedian Technical Assistance Center
             Accedian Networks, Inc.
             2351 Alfred-Nobel blvd., Suite N-410
             Saint-Laurent, Quebec Canada H4S 2A9
             E-mail: support@accedian.com"
    DESCRIPTION
            "This MIB is complementary to the IEEE P802.1ag(TM) CFM MIB. It
             covers the delay measurment and the packet loss configuration
             and results."

    REVISION "201609230100Z"        -- 23 September 2016
    DESCRIPTION
            "Add the history indexes to the corresponding OBJECT-GROUPs.
             Remove acdCfmCfgIfAssignInstIdx out of acdCfmCfgIfAssignGroup.
             Correct the description of acdCfmCfgIfAssignGroup."

    REVISION "201607050100Z"        -- 05 July 2016
    DESCRIPTION
            "Set acdCfmSlmHistResultPeriodIndex instead of
             acdCfmSlmHistResultInstanceIndex as the index for
             acdCfmSlmHistResultTable."

    REVISION "201605260100Z"        -- 26 May 2016
    DESCRIPTION
            "Set access level to read-only for acdCfmHistResultOneWayDelayID,
             acdCfmHistResultOneWayDelaySampleIndex, acdCfmHistResultOneWayDvID,
             acdCfmHistResultOneWayDvSampleIndex, acdCfmHistResultTwoWayDelayID,
             acdCfmHistResultTwoWayDelaySampleIndex, acdCfmHistResultTwoWayDvID,
             acdCfmHistResultTwoWayDvSampleIndex, acdCfmHistResultPktLossID,
             acdCfmHistResultPktLossSampleIndex, acdCfmSlmHistResultID,
             acdCfmSlmHistResultInstanceIndex."

    REVISION "201407040100Z"        -- 04 July 2014
    DESCRIPTION
            "Add InterfaceStatusTLVEnable to acdCfmMepCfgTable."

    REVISION "201301070100Z"        -- 07 January 2013
    DESCRIPTION
            "Add configured name for statistics and history tables."

    REVISION "201204100100Z"        -- 10 April 2012
    DESCRIPTION
            "Add support for invalid CSF PDU counters."

    REVISION "201201180100Z"        -- 18 Jan 2012
    DESCRIPTION
            "Add support for configuration of MEP instance."

    REVISION "201201090100Z"        -- 09 Jan 2012
    DESCRIPTION
            "Add support for DMM and Pkt-Loss instance naming."


    REVISION "201112210100Z"        -- 21 Dec 2011
    DESCRIPTION
            "Add support for ETH-SLM Tx/Rx PDU counters."


    REVISION "201112200100Z"        -- 20 Dec 2011
    DESCRIPTION
            "Add support for ETH-CSF Tx/Rx PDU counters."


    REVISION "201109210100Z"        -- 21 Sept 2011
    DESCRIPTION
            "Add support for CFM Stack Table."

    REVISION "201103300100Z"        -- 30 Mars 2011
    DESCRIPTION
            "Add support for Instantaneous values."

    REVISION "200911010100Z"        -- 1 Nov 2009
    DESCRIPTION
            "Add support for extended packet loss ratio."

    REVISION "200902230100Z"        -- 23 Feb 2009
    DESCRIPTION
            "Add support for extended packet loss ratio."

    REVISION "200805010100Z"        -- 1 May 2008
    DESCRIPTION
            "Initial version of MIB module ACD-CFM-MIB."

    ::= { acdMibs 7 }

acdCfmNotifications     OBJECT IDENTIFIER ::= { acdCfm 0 }
acdCfmMIBObjects        OBJECT IDENTIFIER ::= { acdCfm 1 }
acdCfmConformance       OBJECT IDENTIFIER ::= { acdCfm 2 }

acdCfmDelayMeasurement  OBJECT IDENTIFIER ::= { acdCfmMIBObjects 1 }
acdCfmPacketLoss        OBJECT IDENTIFIER ::= { acdCfmMIBObjects 2 }
acdCfmMep               OBJECT IDENTIFIER ::= { acdCfmMIBObjects 3 }
acdCfmStack             OBJECT IDENTIFIER ::= { acdCfmMIBObjects 4 }
acdCfmSlm               OBJECT IDENTIFIER ::= { acdCfmMIBObjects 5 }
acdCfmConfig            OBJECT IDENTIFIER ::= { acdCfmMIBObjects 6 }

-- ******************************************************************
-- Textual conventions
-- ******************************************************************
AcdCfmMepDirection ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "Indicates the direction in which the Maintenance
        association (MEP) faces on the bridge port:

        down(1)    Sends Continuity Check Messages away from the
                   MAC Relay Entity.
        up(2)      Sends Continuity Check Messages towards the
                   MAC Relay Entity.
       "
    SYNTAX      INTEGER {
                  down  (1),
                  up    (2)
                }

AcdCfmMepLowestAlarmPri ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "An integer value specifying the lowest priority defect
        that is allowed to generate a Fault Alarm (20.9.5), either:

        soamAll(1)           DefRDICCM, DefMACstatus, DefRemoteCCM,
                            DefErrorCCM, and DefXconCCM;
        soamMacRemErrXcon(2)    Only DefMACstatus, DefRemoteCCM,
                            DefErrorCCM, and DefXconCCM (default);
        soamRemErrXcon(3)       Only DefRemoteCCM, DefErrorCCM,
                            and DefXconCCM;
        soamErrXcon(4)          Only DefErrorCCM and DefXconCCM;
        soamXcon(5)             Only DefXconCCM; or
        soamAis(6)           No defects DefXcon or lower are to be
                            reported
        soamNone(7)             No defects will be reported"
    SYNTAX      INTEGER {
                  soamAll              (1),
                  soamMacRemErrXcon (2),
                  soamRemErrXcon     (3),
                  soamErrXcon         (4),
                  soamXcon             (5),
                  soamAis              (6),
                  soamNone             (7)
                }

AcdCfmInterfaceAssign ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "Indicates the assignment configuration/state of a system interface

        unassigned(1)    Interface has not been assigned to a cfm
        assigned(2)      Interface has been assigned to a cfm
       "
    SYNTAX      INTEGER {
                  unassigned  (1),
                  assigned    (2)
                }



---------------------------------------------------------------------------
 -- The Delay Measurement configuration table
 -- This table contains all Delay Measurement entry configurations.
---------------------------------------------------------------------------

acdCfmDmCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmDmCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of all DM entries."
    ::= { acdCfmDelayMeasurement 1 }

acdCfmDmCfgEntry OBJECT-TYPE
    SYNTAX      AcdCfmDmCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all settings to manage a DM instance."
    INDEX   { acdCfmDmCfgID }
    ::=  { acdCfmDmCfgTable 1 }

AcdCfmDmCfgEntry ::= SEQUENCE {
    acdCfmDmCfgID                       Unsigned32,
    acdCfmDmCfgRowStatus                RowStatus,
    acdCfmDmCfgMepIdx                   Unsigned32,
    acdCfmDmCfgRemoteMepId              Unsigned32,
    acdCfmDmCfgPriority                 Unsigned32,
    acdCfmDmCfgEnable                   TruthValue,
    acdCfmDmCfgInterval                 Unsigned32,
    acdCfmDmCfgRefPeriod                Unsigned32,
    acdCfmDmCfgOneWayDelayEnable        TruthValue,
    acdCfmDmCfgOneWayDelayMax           Unsigned32,
    acdCfmDmCfgOneWayDelayThresh        Unsigned32,
    acdCfmDmCfgOneWayAvgDelayThresh     Unsigned32,
    acdCfmDmCfgOneWayDvEnable           TruthValue,
    acdCfmDmCfgOneWayDvMax              Unsigned32,
    acdCfmDmCfgOneWayDvThresh           Unsigned32,
    acdCfmDmCfgOneWayAvgDvThresh        Unsigned32,
    acdCfmDmCfgTwoWayDelayEnable        TruthValue,
    acdCfmDmCfgTwoWayDelayMax           Unsigned32,
    acdCfmDmCfgTwoWayDelayThresh        Unsigned32,
    acdCfmDmCfgTwoWayAvgDelayThresh     Unsigned32,
    acdCfmDmCfgTwoWayDvEnable           TruthValue,
    acdCfmDmCfgTwoWayDvMax              Unsigned32,
    acdCfmDmCfgTwoWayDvThresh           Unsigned32,
    acdCfmDmCfgTwoWayAvgDvThresh        Unsigned32,
    acdCfmDmCfgName                     DisplayString
}

acdCfmDmCfgID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the results table."
    ::= { acdCfmDmCfgEntry 1 }

acdCfmDmCfgRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "All columns must have a valid value before a row can be activated."
    ::= { acdCfmDmCfgEntry 2 }

acdCfmDmCfgMepIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maintenance association End Point Identifier."
    ::= { acdCfmDmCfgEntry 3 }

acdCfmDmCfgRemoteMepId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Remote Maintenance association End Point Identifier used for this
         delay measurement configuration."
    ::= { acdCfmDmCfgEntry 4 }

acdCfmDmCfgPriority  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..7)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VLAN priority. Its value ranges from 0 to 7."
    DEFVAL      { 0 }
    ::= { acdCfmDmCfgEntry 5 }

acdCfmDmCfgEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to issues DMM measurement packets."
    DEFVAL      { false }
    ::= { acdCfmDmCfgEntry 6 }

acdCfmDmCfgInterval  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Interval in milliseconds at which CFM issues DMM measurement packets."
    DEFVAL      { 10000 }
    ::= { acdCfmDmCfgEntry 7 }

acdCfmDmCfgRefPeriod  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..1440)
    UNITS       "minutes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Reference period in minutes for Delay Measurement."
    DEFVAL      { 15 }
    ::= { acdCfmDmCfgEntry 8 }

acdCfmDmCfgOneWayDelayEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to compute one-way delay measurements."
    DEFVAL      { true }
    ::= { acdCfmDmCfgEntry 9 }

acdCfmDmCfgOneWayDelayMax  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum allowed instantaneous delay in milliseconds."
     DEFVAL      { 50 }
    ::= { acdCfmDmCfgEntry 10 }

acdCfmDmCfgOneWayDelayThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Number of consecutive delay greater than the maximum allowed value
        before alert."
     DEFVAL      { 4 }
   ::= { acdCfmDmCfgEntry 11 }

acdCfmDmCfgOneWayAvgDelayThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "One-way average delay threshold in milliseconds."
     DEFVAL      { 50 }
    ::= { acdCfmDmCfgEntry 12 }

acdCfmDmCfgOneWayDvEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to compute one-way delay variation measurements."
    DEFVAL      { true }
    ::= { acdCfmDmCfgEntry 13 }

acdCfmDmCfgOneWayDvMax  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum allowed instantaneous delay variation in milliseconds."
     DEFVAL      { 50 }
    ::= { acdCfmDmCfgEntry 14 }

acdCfmDmCfgOneWayDvThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Number of consecutive delay variation greater than the maximum
        allowed value before alert."
     DEFVAL      { 10 }
    ::= { acdCfmDmCfgEntry 15 }

acdCfmDmCfgOneWayAvgDvThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "One-way average delay variation threshold in milliseconds."
     DEFVAL      { 4 }
    ::= { acdCfmDmCfgEntry 16 }

acdCfmDmCfgTwoWayDelayEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to compute Two-way delay measurements."
    DEFVAL      { true }
    ::= { acdCfmDmCfgEntry 17 }

acdCfmDmCfgTwoWayDelayMax  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum allowed instantaneous delay in milliseconds."
      DEFVAL      { 100 }
   ::= { acdCfmDmCfgEntry 18 }

acdCfmDmCfgTwoWayDelayThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Number of consecutive delay greater than the maximum allowed value
        before alert."
     DEFVAL      { 40 }
    ::= { acdCfmDmCfgEntry 19 }

acdCfmDmCfgTwoWayAvgDelayThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Two-way average delay threshold in milliseconds."
     DEFVAL      { 100 }
    ::= { acdCfmDmCfgEntry 20 }

acdCfmDmCfgTwoWayDvEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to compute Two-way delay variation measurements."
    DEFVAL      { true }
    ::= { acdCfmDmCfgEntry 21 }

acdCfmDmCfgTwoWayDvMax  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum allowed instantaneous delay variation in milliseconds."
     DEFVAL      { 10 }
    ::= { acdCfmDmCfgEntry 22 }

acdCfmDmCfgTwoWayDvThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Number of consecutive delay variation greater than the maximum
        allowed value before alert."
     DEFVAL      { 4 }
    ::= { acdCfmDmCfgEntry 23 }

acdCfmDmCfgTwoWayAvgDvThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Two-way average delay variation threshold in milliseconds."
     DEFVAL      { 10 }
    ::= { acdCfmDmCfgEntry 24 }

acdCfmDmCfgName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmDmCfgEntry 25 }


---------------------------------------------------------------------------
 -- The CFM DMM One Way delay Results table
 -- This table contains all CFM DMM One Way delay entry results.
---------------------------------------------------------------------------

acdCfmResultOneWayDelayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmResultOneWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "One way delay result table of all DM entries."
    ::= { acdCfmDelayMeasurement 2 }

acdCfmResultOneWayDelayEntry OBJECT-TYPE
    SYNTAX      AcdCfmResultOneWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of One Way Delay results for a DM entry."
    INDEX   { acdCfmResultOneWayDelayID }
    ::=  { acdCfmResultOneWayDelayTable 1 }

AcdCfmResultOneWayDelayEntry ::= SEQUENCE {
    acdCfmResultOneWayDelayID               Unsigned32,
    acdCfmResultOneWayDelayPeriodIndex      Unsigned32,
    acdCfmResultOneWayDelayIntervalStart    DateAndTime,
    acdCfmResultOneWayDelayValid            TruthValue,
    acdCfmResultOneWayDelayAlert            TruthValue,
    acdCfmResultOneWayDelayAvgAlert         TruthValue,
    acdCfmResultOneWayDelaySamples          Unsigned32,
    acdCfmResultOneWayDelayMinValue         Integer32,
    acdCfmResultOneWayDelayMaxValue         Integer32,
    acdCfmResultOneWayDelayAvgValue         Integer32,
    acdCfmResultOneWayDelayThreshExc        Unsigned32,
    acdCfmResultOneWayDelayInstValue        Integer32,
    acdCfmResultOneWayDelayName             DisplayString
}

acdCfmResultOneWayDelayID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the Dm table."
    ::= { acdCfmResultOneWayDelayEntry 1 }

acdCfmResultOneWayDelayPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmResultOneWayDelayEntry 2 }

acdCfmResultOneWayDelayIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmResultOneWayDelayEntry 3 }

acdCfmResultOneWayDelayValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the One-way delay results during this
        sampling interval."
    ::= { acdCfmResultOneWayDelayEntry 4 }

acdCfmResultOneWayDelayAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the One Way Delay alert."
    ::= { acdCfmResultOneWayDelayEntry 5 }

acdCfmResultOneWayDelayAvgAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the One Way Average Delay alert."
    ::= { acdCfmResultOneWayDelayEntry 6 }

acdCfmResultOneWayDelaySamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate One-way delay results."
    ::= { acdCfmResultOneWayDelayEntry 7 }

acdCfmResultOneWayDelayMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultOneWayDelayEntry 8 }

acdCfmResultOneWayDelayMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultOneWayDelayEntry 9 }

acdCfmResultOneWayDelayAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultOneWayDelayEntry 10}

acdCfmResultOneWayDelayThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmResultOneWayDelayEntry 11 }

acdCfmResultOneWayDelayInstValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay Instantaneous value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultOneWayDelayEntry 12 }

acdCfmResultOneWayDelayName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique string used to identify this instance."

    ::= { acdCfmResultOneWayDelayEntry 13 }

---------------------------------------------------------------------------
 -- The CFM DMM One Way delay variation Results table
 -- This table contains all CFM DMM One Way delay variation entry results.
---------------------------------------------------------------------------

acdCfmResultOneWayDvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmResultOneWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "One way delay variation result table of all DM entries."
    ::= { acdCfmDelayMeasurement 3 }

acdCfmResultOneWayDvEntry OBJECT-TYPE
    SYNTAX      AcdCfmResultOneWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of One Way Delay variation results for a DM entry."
    INDEX   { acdCfmResultOneWayDvID }
    ::=  { acdCfmResultOneWayDvTable 1 }

AcdCfmResultOneWayDvEntry ::= SEQUENCE {
    acdCfmResultOneWayDvID              Unsigned32,
    acdCfmResultOneWayDvPeriodIndex     Unsigned32,
    acdCfmResultOneWayDvIntervalStart   DateAndTime,
    acdCfmResultOneWayDvValid           TruthValue,
    acdCfmResultOneWayDvAlert           TruthValue,
    acdCfmResultOneWayDvAvgAlert        TruthValue,
    acdCfmResultOneWayDvSamples         Unsigned32,
    acdCfmResultOneWayDvMinValue        Integer32,
    acdCfmResultOneWayDvMaxValue        Integer32,
    acdCfmResultOneWayDvAvgValue        Integer32,
    acdCfmResultOneWayDvThreshExc       Unsigned32,
    acdCfmResultOneWayDvInstValue       Integer32,
    acdCfmResultOneWayDvName            DisplayString
}

acdCfmResultOneWayDvID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This value follows
        the ordering of the DM table."
    ::= { acdCfmResultOneWayDvEntry 1 }

acdCfmResultOneWayDvPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmResultOneWayDvEntry 2 }

acdCfmResultOneWayDvIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmResultOneWayDvEntry 3 }

acdCfmResultOneWayDvValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the One-way delay variation results during this
        sampling interval."
    ::= { acdCfmResultOneWayDvEntry 4 }

acdCfmResultOneWayDvAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the One Way Delay variation alert."
    ::= { acdCfmResultOneWayDvEntry 5 }

acdCfmResultOneWayDvAvgAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the One Way Average Delay variation alert."
    ::= { acdCfmResultOneWayDvEntry 6 }

acdCfmResultOneWayDvSamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate One-way delay variation results."
    ::= { acdCfmResultOneWayDvEntry 7 }

acdCfmResultOneWayDvMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variation minimum value. The value is
        expressed in micro-seconds."
    ::= { acdCfmResultOneWayDvEntry 8 }

acdCfmResultOneWayDvMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variationmaximum value. The value is
        expressed in micro-seconds."
    ::= { acdCfmResultOneWayDvEntry 9 }

acdCfmResultOneWayDvAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variation average value. The value is
        expressed in micro-seconds."
    ::= { acdCfmResultOneWayDvEntry 10}

acdCfmResultOneWayDvThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmResultOneWayDvEntry 11 }

acdCfmResultOneWayDvInstValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variation Instantaneous value. The value is
        expressed in micro-seconds."
    ::= { acdCfmResultOneWayDvEntry 12 }

acdCfmResultOneWayDvName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique string used to identify this instance. The length includes the terminating NULL character."

    ::= { acdCfmResultOneWayDvEntry 13 }


---------------------------------------------------------------------------
 -- The CFM DMM Two Way delay Results table
 -- This table contains all CFM DMM Two Way delay entry results.
---------------------------------------------------------------------------

acdCfmResultTwoWayDelayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmResultTwoWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Two way delay result table of all DM entries."
    ::= { acdCfmDelayMeasurement 4 }

acdCfmResultTwoWayDelayEntry OBJECT-TYPE
    SYNTAX      AcdCfmResultTwoWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of Two Way Delay results for a DM entry."
    INDEX   { acdCfmResultTwoWayDelayID }
    ::=  { acdCfmResultTwoWayDelayTable 1 }

AcdCfmResultTwoWayDelayEntry ::= SEQUENCE {
    acdCfmResultTwoWayDelayID               Unsigned32,
    acdCfmResultTwoWayDelayPeriodIndex      Unsigned32,
    acdCfmResultTwoWayDelayIntervalStart    DateAndTime,
    acdCfmResultTwoWayDelayValid            TruthValue,
    acdCfmResultTwoWayDelayAlert            TruthValue,
    acdCfmResultTwoWayDelayAvgAlert         TruthValue,
    acdCfmResultTwoWayDelaySamples          Unsigned32,
    acdCfmResultTwoWayDelayMinValue         Integer32,
    acdCfmResultTwoWayDelayMaxValue         Integer32,
    acdCfmResultTwoWayDelayAvgValue         Integer32,
    acdCfmResultTwoWayDelayThreshExc        Unsigned32,
    acdCfmResultTwoWayDelayInstValue        Integer32,
    acdCfmResultTwoWayDelayName             DisplayString
}

acdCfmResultTwoWayDelayID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the Dm table."
    ::= { acdCfmResultTwoWayDelayEntry 1 }

acdCfmResultTwoWayDelayPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmResultTwoWayDelayEntry 2 }

acdCfmResultTwoWayDelayIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmResultTwoWayDelayEntry 3 }

acdCfmResultTwoWayDelayValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the Two way delay results during this
        sampling interval."
    ::= { acdCfmResultTwoWayDelayEntry 4 }

acdCfmResultTwoWayDelayAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the Two Way Delay alert."
    ::= { acdCfmResultTwoWayDelayEntry 5 }

acdCfmResultTwoWayDelayAvgAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the Two Way Average Delay alert."
    ::= { acdCfmResultTwoWayDelayEntry 6 }

acdCfmResultTwoWayDelaySamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate Two-way delay results."
    ::= { acdCfmResultTwoWayDelayEntry 7 }

acdCfmResultTwoWayDelayMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDelayEntry 8 }

acdCfmResultTwoWayDelayMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDelayEntry 9 }

acdCfmResultTwoWayDelayAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDelayEntry 10}

acdCfmResultTwoWayDelayThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmResultTwoWayDelayEntry 11 }

acdCfmResultTwoWayDelayInstValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay Instantaneous value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDelayEntry 12 }

acdCfmResultTwoWayDelayName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique string used to identify this instance. The length includes the terminating NULL character."

    ::= { acdCfmResultTwoWayDelayEntry 13 }


---------------------------------------------------------------------------
 -- The CFM DMM Two Way delay variation Results table
 -- This table contains all CFM DMM Two Way delay variation entry results.
---------------------------------------------------------------------------

acdCfmResultTwoWayDvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmResultTwoWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Two way delay variation result table of all DM entries."
    ::= { acdCfmDelayMeasurement 5 }

acdCfmResultTwoWayDvEntry OBJECT-TYPE
    SYNTAX      AcdCfmResultTwoWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of One Way Delay variation results for a DM entry."
    INDEX   { acdCfmResultTwoWayDvID }
    ::=  { acdCfmResultTwoWayDvTable 1 }

AcdCfmResultTwoWayDvEntry ::= SEQUENCE {
    acdCfmResultTwoWayDvID               Unsigned32,
    acdCfmResultTwoWayDvPeriodIndex      Unsigned32,
    acdCfmResultTwoWayDvIntervalStart    DateAndTime,
    acdCfmResultTwoWayDvValid            TruthValue,
    acdCfmResultTwoWayDvAlert            TruthValue,
    acdCfmResultTwoWayDvAvgAlert         TruthValue,
    acdCfmResultTwoWayDvSamples          Unsigned32,
    acdCfmResultTwoWayDvMinValue         Integer32,
    acdCfmResultTwoWayDvMaxValue         Integer32,
    acdCfmResultTwoWayDvAvgValue         Integer32,
    acdCfmResultTwoWayDvThreshExc        Unsigned32,
    acdCfmResultTwoWayDvInstValue        Integer32, 
    acdCfmResultTwoWayDvName             DisplayString
}

acdCfmResultTwoWayDvID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This
        value follows the ordering of the Dm table."
    ::= { acdCfmResultTwoWayDvEntry 1 }

acdCfmResultTwoWayDvPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmResultTwoWayDvEntry 2 }

acdCfmResultTwoWayDvIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmResultTwoWayDvEntry 3 }

acdCfmResultTwoWayDvValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the two-way delay variation results during this
        sampling interval."
    ::= { acdCfmResultTwoWayDvEntry 4 }

acdCfmResultTwoWayDvAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the Two Way Delay variation alert."
    ::= { acdCfmResultTwoWayDvEntry 5 }

acdCfmResultTwoWayDvAvgAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the Two Way Average Delay variation alert."
    ::= { acdCfmResultTwoWayDvEntry 6 }

acdCfmResultTwoWayDvSamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate Two-way delay variation results."
    ::= { acdCfmResultTwoWayDvEntry 7 }

acdCfmResultTwoWayDvMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDvEntry 8 }

acdCfmResultTwoWayDvMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDvEntry 9 }

acdCfmResultTwoWayDvAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmResultTwoWayDvEntry 10}

acdCfmResultTwoWayDvThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmResultTwoWayDvEntry 11 }

acdCfmResultTwoWayDvInstValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation Instantaneous value. The value is
        expressed in micro-seconds."
    ::= { acdCfmResultTwoWayDvEntry 12 }

acdCfmResultTwoWayDvName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique string used to identify this instance. The length includes the terminating NULL character."

    ::= { acdCfmResultTwoWayDvEntry 13 }

---------------------------------------------------------------------------
 -- The CFM DMM One Way delay History Results table
 -- This table contains all CFM DMM One Way delay entry History results.
---------------------------------------------------------------------------

acdCfmHistResultOneWayDelayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmHistResultOneWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "One way delay result table of all DM entries."
    ::= { acdCfmDelayMeasurement 6 }

acdCfmHistResultOneWayDelayEntry OBJECT-TYPE
    SYNTAX      AcdCfmHistResultOneWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of One Way Delay results for a DM entry."
    INDEX   { acdCfmHistResultOneWayDelayID,
              acdCfmHistResultOneWayDelaySampleIndex }
    ::=  { acdCfmHistResultOneWayDelayTable 1 }

AcdCfmHistResultOneWayDelayEntry ::= SEQUENCE {
    acdCfmHistResultOneWayDelayID               Unsigned32,
    acdCfmHistResultOneWayDelaySampleIndex      Unsigned32,
    acdCfmHistResultOneWayDelayStatus           INTEGER,
    acdCfmHistResultOneWayDelayDuration         Unsigned32,
    acdCfmHistResultOneWayDelayIntervalEnd      DateAndTime,
    acdCfmHistResultOneWayDelaySamples          Unsigned32,
    acdCfmHistResultOneWayDelayMinValue         Integer32,
    acdCfmHistResultOneWayDelayMaxValue         Integer32,
    acdCfmHistResultOneWayDelayAvgValue         Integer32,
    acdCfmHistResultOneWayDelayThreshExc        Unsigned32,
    acdCfmHistResultOneWayDelayName             DisplayString
}

acdCfmHistResultOneWayDelayID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the Dm table."
    ::= { acdCfmHistResultOneWayDelayEntry 1 }

acdCfmHistResultOneWayDelaySampleIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmHistResultOneWayDelayEntry 2 }

acdCfmHistResultOneWayDelayStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(1),
                    invalid(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the One-way delay results during this
        sampling interval."
    ::= { acdCfmHistResultOneWayDelayEntry 3 }

acdCfmHistResultOneWayDelayDuration  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the Dm table."
    ::= { acdCfmHistResultOneWayDelayEntry 4 }

acdCfmHistResultOneWayDelayIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of the period."
    ::= { acdCfmHistResultOneWayDelayEntry 5 }


acdCfmHistResultOneWayDelaySamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate One-way delay results."
    ::= { acdCfmHistResultOneWayDelayEntry 6 }

acdCfmHistResultOneWayDelayMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultOneWayDelayEntry 7 }

acdCfmHistResultOneWayDelayMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultOneWayDelayEntry 8 }

acdCfmHistResultOneWayDelayAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultOneWayDelayEntry 9}

acdCfmHistResultOneWayDelayThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmHistResultOneWayDelayEntry 10 }

acdCfmHistResultOneWayDelayName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmHistResultOneWayDelayEntry 11 }

---------------------------------------------------------------------------
 -- The CFM DMM One Way delay variation History Results table
 -- This table contains all CFM DMM One Way delay variation entry History results.
---------------------------------------------------------------------------

acdCfmHistResultOneWayDvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmHistResultOneWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "One way delay variation result table of all DM entries."
    ::= { acdCfmDelayMeasurement 7 }

acdCfmHistResultOneWayDvEntry OBJECT-TYPE
    SYNTAX      AcdCfmHistResultOneWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of One Way Delay variation results for a DM entry."
    INDEX   { acdCfmHistResultOneWayDvID,
              acdCfmHistResultOneWayDvSampleIndex }
    ::=  { acdCfmHistResultOneWayDvTable 1 }

AcdCfmHistResultOneWayDvEntry ::= SEQUENCE {
    acdCfmHistResultOneWayDvID              Unsigned32,
    acdCfmHistResultOneWayDvSampleIndex     Unsigned32,
    acdCfmHistResultOneWayDvStatus          INTEGER,
    acdCfmHistResultOneWayDvDuration        Unsigned32,
    acdCfmHistResultOneWayDvIntervalEnd     DateAndTime,
    acdCfmHistResultOneWayDvSamples         Unsigned32,
    acdCfmHistResultOneWayDvMinValue        Integer32,
    acdCfmHistResultOneWayDvMaxValue        Integer32,
    acdCfmHistResultOneWayDvAvgValue        Integer32,
    acdCfmHistResultOneWayDvThreshExc       Unsigned32,
    acdCfmHistResultOneWayDvName            DisplayString
}


acdCfmHistResultOneWayDvID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This value follows
        the ordering of the DM table."
    ::= { acdCfmHistResultOneWayDvEntry 1 }

acdCfmHistResultOneWayDvSampleIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmHistResultOneWayDvEntry 2 }

acdCfmHistResultOneWayDvStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(1),
                    invalid(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the One-way delay variation results during this
        sampling interval."
    ::= { acdCfmHistResultOneWayDvEntry 3 }

acdCfmHistResultOneWayDvDuration  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interval in seconds over which the data is sampled for this entry."
    ::= { acdCfmHistResultOneWayDvEntry 4 }

acdCfmHistResultOneWayDvIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of the period."
    ::= { acdCfmHistResultOneWayDvEntry 5 }

acdCfmHistResultOneWayDvSamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate One-way delay variation results."
    ::= { acdCfmHistResultOneWayDvEntry 6 }

acdCfmHistResultOneWayDvMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variation minimum value. The value is
        expressed in micro-seconds."
    ::= { acdCfmHistResultOneWayDvEntry 7 }

acdCfmHistResultOneWayDvMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variationmaximum value. The value is
        expressed in micro-seconds."
    ::= { acdCfmHistResultOneWayDvEntry 8 }

acdCfmHistResultOneWayDvAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the One-way delay variation average value. The value is
        expressed in micro-seconds."
    ::= { acdCfmHistResultOneWayDvEntry 9 }

acdCfmHistResultOneWayDvThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmHistResultOneWayDvEntry 10 }

acdCfmHistResultOneWayDvName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmHistResultOneWayDvEntry 11 }

---------------------------------------------------------------------------
 -- The CFM DMM Two Way delay History Results table
 -- This table contains all CFM DMM Two Way delay entry History results.
---------------------------------------------------------------------------

acdCfmHistResultTwoWayDelayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmHistResultTwoWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Two way delay result table of all DM entries."
    ::= { acdCfmDelayMeasurement 8 }

acdCfmHistResultTwoWayDelayEntry OBJECT-TYPE
    SYNTAX      AcdCfmHistResultTwoWayDelayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of Two Way Delay results for a DM entry."
    INDEX   { acdCfmHistResultTwoWayDelayID,
              acdCfmHistResultTwoWayDelaySampleIndex }
    ::=  { acdCfmHistResultTwoWayDelayTable 1 }

AcdCfmHistResultTwoWayDelayEntry ::= SEQUENCE {
    acdCfmHistResultTwoWayDelayID               Unsigned32,
    acdCfmHistResultTwoWayDelaySampleIndex      Unsigned32,
    acdCfmHistResultTwoWayDelayStatus           INTEGER,
    acdCfmHistResultTwoWayDelayDuration         Unsigned32,
    acdCfmHistResultTwoWayDelayIntervalEnd      DateAndTime,
    acdCfmHistResultTwoWayDelaySamples          Unsigned32,
    acdCfmHistResultTwoWayDelayMinValue         Integer32,
    acdCfmHistResultTwoWayDelayMaxValue         Integer32,
    acdCfmHistResultTwoWayDelayAvgValue         Integer32,
    acdCfmHistResultTwoWayDelayThreshExc        Unsigned32,
    acdCfmHistResultTwoWayDelayName             DisplayString
}

acdCfmHistResultTwoWayDelayID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay Measurement instance. This value follows
        the ordering of the Dm table."
    ::= { acdCfmHistResultTwoWayDelayEntry 1 }

acdCfmHistResultTwoWayDelaySampleIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmHistResultTwoWayDelayEntry 2 }

acdCfmHistResultTwoWayDelayStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(1),
                    invalid(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the Two way delay results during this
        sampling interval."
    ::= { acdCfmHistResultTwoWayDelayEntry 3 }

acdCfmHistResultTwoWayDelayDuration  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interval in seconds over which the data is sampled for this entry."
    ::= { acdCfmHistResultTwoWayDelayEntry 4 }

acdCfmHistResultTwoWayDelayIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of the period."
    ::= { acdCfmHistResultTwoWayDelayEntry 5 }

acdCfmHistResultTwoWayDelaySamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate Two-way delay results."
    ::= { acdCfmHistResultTwoWayDelayEntry 6 }

acdCfmHistResultTwoWayDelayMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDelayEntry 7 }

acdCfmHistResultTwoWayDelayMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDelayEntry 8 }

acdCfmHistResultTwoWayDelayAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Two-way delay average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDelayEntry 9 }

acdCfmHistResultTwoWayDelayThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmHistResultTwoWayDelayEntry 10 }

acdCfmHistResultTwoWayDelayName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmHistResultTwoWayDelayEntry 11 }


---------------------------------------------------------------------------
 -- The CFM DMM Two Way delay variation History Results table
 -- This table contains all CFM DMM Two Way delay variation entry History results.
---------------------------------------------------------------------------

acdCfmHistResultTwoWayDvTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmHistResultTwoWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Two way delay variation result table of all DM entries."
    ::= { acdCfmDelayMeasurement 9 }

acdCfmHistResultTwoWayDvEntry OBJECT-TYPE
    SYNTAX      AcdCfmHistResultTwoWayDvEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of two Way Delay variation results for a DM entry."
    INDEX   { acdCfmHistResultTwoWayDvID,
              acdCfmHistResultTwoWayDvSampleIndex }
    ::=  { acdCfmHistResultTwoWayDvTable 1 }

AcdCfmHistResultTwoWayDvEntry ::= SEQUENCE {
    acdCfmHistResultTwoWayDvID               Unsigned32,
    acdCfmHistResultTwoWayDvSampleIndex      Unsigned32,
    acdCfmHistResultTwoWayDvStatus           INTEGER,
    acdCfmHistResultTwoWayDvDuration         Unsigned32,
    acdCfmHistResultTwoWayDvIntervalEnd      DateAndTime,
    acdCfmHistResultTwoWayDvSamples          Unsigned32,
    acdCfmHistResultTwoWayDvMinValue         Integer32,
    acdCfmHistResultTwoWayDvMaxValue         Integer32,
    acdCfmHistResultTwoWayDvAvgValue         Integer32,
    acdCfmHistResultTwoWayDvThreshExc        Unsigned32,
    acdCfmHistResultTwoWayDvName             DisplayString
}

acdCfmHistResultTwoWayDvID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This
        value follows the ordering of the Dm table."
    ::= { acdCfmHistResultTwoWayDvEntry 1 }

acdCfmHistResultTwoWayDvSampleIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same DM instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmHistResultTwoWayDvEntry 2 }

acdCfmHistResultTwoWayDvStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(1),
                    invalid(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the two-way delay variation results during this
        sampling interval."
    ::= { acdCfmHistResultTwoWayDvEntry 3 }

acdCfmHistResultTwoWayDvDuration  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interval in seconds over which the data is sampled for this entry."
    ::= { acdCfmHistResultTwoWayDvEntry 4 }

acdCfmHistResultTwoWayDvIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of the period."
    ::= { acdCfmHistResultTwoWayDvEntry 5 }

acdCfmHistResultTwoWayDvSamples  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate Two-way delay variation results."
    ::= { acdCfmHistResultTwoWayDvEntry 6 }

acdCfmHistResultTwoWayDvMinValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation minimum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDvEntry 7 }

acdCfmHistResultTwoWayDvMaxValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation maximum value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDvEntry 8 }

acdCfmHistResultTwoWayDvAvgValue  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "microseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the two-way delay variation average value. The value is expressed in
        micro-seconds."
    ::= { acdCfmHistResultTwoWayDvEntry 9 }

acdCfmHistResultTwoWayDvThreshExc  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples exceeding the limit."
    ::= { acdCfmHistResultTwoWayDvEntry 10 }

acdCfmHistResultTwoWayDvName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmHistResultTwoWayDvEntry 11 }


---------------------------------------------------------------------------
 -- The Packet Loss configuration table
 -- This table contains all Packet Loss entry configurations.
---------------------------------------------------------------------------

acdCfmPktLossCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmPktLossCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of all Packet Loss entries."
    ::= { acdCfmPacketLoss 1 }

acdCfmPktLossCfgEntry OBJECT-TYPE
    SYNTAX      AcdCfmPktLossCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all settings to manage a Packet loss instance."
    INDEX   { acdCfmPktLossCfgID }
    ::=  { acdCfmPktLossCfgTable 1 }


AcdCfmPktLossCfgEntry ::= SEQUENCE {
    acdCfmPktLossCfgID              Unsigned32,
    acdCfmPktLossCfgRowStatus       RowStatus,
    acdCfmPktLossCfgMepIdx          Unsigned32,
    acdCfmPktLossCfgRemoteMepId     Unsigned32,
    acdCfmPktLossCfgPriority        Unsigned32,
    acdCfmPktLossCfgEnable          TruthValue,
    acdCfmPktLossCfgInterval        Unsigned32,
    acdCfmPktLossCfgRefPeriod       Unsigned32,
    acdCfmPktLossCfgThresh          Unsigned32,
    acdCfmPktLossCfgRatioThresh     Unsigned32,
    acdCfmPktLossCfgName            DisplayString
}

acdCfmPktLossCfgID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Packet Loss instance. This value follows the
         ordering the results table."
    ::= { acdCfmPktLossCfgEntry 1 }

acdCfmPktLossCfgRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The writable columns in a row can not be changed if the row is active.
       All columns must have a valid value before a row can be activated."
    ::= { acdCfmPktLossCfgEntry 2 }

acdCfmPktLossCfgMepIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maintenance association End Point Identifier."
    ::= { acdCfmPktLossCfgEntry 3 }

acdCfmPktLossCfgRemoteMepId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Remote Maintenance association End Point Identifier."
    ::= { acdCfmPktLossCfgEntry 4 }

acdCfmPktLossCfgPriority  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..7)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The VLAN priority. Its value ranges from 0 to 7. Same has CCM
         priority for packet loss based on CCM."
     DEFVAL      { 0 }
    ::= { acdCfmPktLossCfgEntry 5 }

acdCfmPktLossCfgEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable CFM to perform Packet Loss measurement."
     DEFVAL      { false }
    ::= { acdCfmPktLossCfgEntry 6 }

acdCfmPktLossCfgInterval  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Interval in milliseconds at which CFM issues Packet Loss measurement
        packets. Same has CCM interval for packet loss based on CCM."
     DEFVAL      { 10000 }
    ::= { acdCfmPktLossCfgEntry 7 }

acdCfmPktLossCfgRefPeriod  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..1440)
    UNITS       "minutes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Reference period in minutes for Packet Loss Measurement."
     DEFVAL      { 15 }
    ::= { acdCfmPktLossCfgEntry 8 }

acdCfmPktLossCfgThresh  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum number of packet loss allowed without issuing an alarm."
     DEFVAL      { 1 }
    ::= { acdCfmPktLossCfgEntry 9 }

acdCfmPktLossCfgRatioThresh  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Packet loss ratio threshold allowed without issuing an alarm
         expressed in millionth of percent (1,000,000 is 1%)."
     DEFVAL      { 0 }
    ::= { acdCfmPktLossCfgEntry 10 }

acdCfmPktLossCfgName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Unique string for each Packet Loss instance. The length includes the terminating NULL character."
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmPktLossCfgEntry 11 }




---------------------------------------------------------------------------
 -- The CFM Packet Loss Results table
 -- This table contains all CFM DMM Packet Loss results.
---------------------------------------------------------------------------

acdCfmResultPktLossTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmResultPktLossEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Packet loss result table of a MEP and remote MEP pair."
    ::= { acdCfmPacketLoss 2 }

acdCfmResultPktLossEntry OBJECT-TYPE
    SYNTAX      AcdCfmResultPktLossEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of packet loss result for a specific MEP and
        remote MEP pair."
    INDEX   { acdCfmResultPktLossID }
    ::=  { acdCfmResultPktLossTable 1 }

AcdCfmResultPktLossEntry ::= SEQUENCE {
    acdCfmResultPktLossID                   Unsigned32,
    acdCfmResultPktLossPeriodIndex          Unsigned32,
    acdCfmResultPktLossIntervalStart        DateAndTime,
    acdCfmResultPktLossValid                TruthValue,
    acdCfmResultPktLossAlert                TruthValue,
    acdCfmResultPktLossSamples              Counter32,
    acdCfmResultPktLossOverflowSamples      Counter32,
    acdCfmResultPktLossHCSamples            Counter64,
    acdCfmResultPktLossNbrLoss              Counter32,
    acdCfmResultPktLossOverflowNbrLoss      Counter32,
    acdCfmResultPktLossHCNbrLoss            Counter64,
    acdCfmResultPktLossNbrGaps              Counter32,
    acdCfmResultPktLossOverflowNbrGaps      Counter32,
    acdCfmResultPktLossHCNbrGaps            Counter64,
    acdCfmResultPktLossLargestGap           Counter32,
    acdCfmResultPktLossOverflowLargestGap   Counter32,
    acdCfmResultPktLossHCLargestGap         Counter64,
    acdCfmResultPktLossRatio                Unsigned32,
    acdCfmResultPktLossName                 DisplayString
}

acdCfmResultPktLossID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This
        value follows the ordering of the Dm table."
    ::= { acdCfmResultPktLossEntry 1 }

acdCfmResultPktLossPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same PL instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmResultPktLossEntry 2 }

acdCfmResultPktLossIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmResultPktLossEntry 3 }

acdCfmResultPktLossValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the packet loss results during this
        sampling interval."
    ::= { acdCfmResultPktLossEntry 4 }

acdCfmResultPktLossAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the Packet Loss alert."
    ::= { acdCfmResultPktLossEntry 5 }

acdCfmResultPktLossSamples  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate packet loss results."
    ::= { acdCfmResultPktLossEntry 6 }

acdCfmResultPktLossOverflowSamples  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmResultPktLossSamples counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmResultPktLossSamples, it provides the equivalent of
         the 64 bits counter acdCfmResultPktLossHCSamples."
    ::= { acdCfmResultPktLossEntry 7 }

acdCfmResultPktLossHCSamples  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate packet loss results."
    ::= { acdCfmResultPktLossEntry 8 }

acdCfmResultPktLossNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of packet loss."
    ::= { acdCfmResultPktLossEntry 9 }

acdCfmResultPktLossOverflowNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmResultPktLossNbrLoss counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmResultPktLossNbrLoss, it provides the equivalent of
         the 64 bits counter acdCfmResultPktLossHCNbrLoss."
    ::= { acdCfmResultPktLossEntry 10 }

acdCfmResultPktLossHCNbrLoss  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of packet loss."
    ::= { acdCfmResultPktLossEntry 11 }

acdCfmResultPktLossNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of gap."
    ::= { acdCfmResultPktLossEntry 12 }

acdCfmResultPktLossOverflowNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmResultPktLossNbrGaps counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmResultPktLossNbrGaps, it provides the equivalent of
         the 64 bits counter acdCfmResultPktLossHCNbrGaps."
    ::= { acdCfmResultPktLossEntry 13 }

acdCfmResultPktLossHCNbrGaps  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of gap."
    ::= { acdCfmResultPktLossEntry 14 }

acdCfmResultPktLossLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "the largest gap size in packets."
    ::= { acdCfmResultPktLossEntry 15 }

acdCfmResultPktLossOverflowLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmResultPktLossLargestGap counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmResultPktLossLargestGap, it provides the equivalent
         of the 64 bits counter acdCfmResultPktLossHCLargestGap."
    ::= { acdCfmResultPktLossEntry 16 }

acdCfmResultPktLossHCLargestGap  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "the largest gap size in packets."
    ::= { acdCfmResultPktLossEntry 17 }

acdCfmResultPktLossRatio  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the packet loss ratio. The packet loss ratio is the percent
         of packets transmitted but not received in millionth of a percent
         (1,000,000 is 1%)."
    ::= { acdCfmResultPktLossEntry 18 }

acdCfmResultPktLossName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each Packet Loss instance. The length includes the terminating NULL character."
    ::= { acdCfmResultPktLossEntry 19 }



---------------------------------------------------------------------------
 -- The CFM Packet Loss History Results table
 -- This table contains all CFM Packet Loss History results.
---------------------------------------------------------------------------

acdCfmHistResultPktLossTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmHistResultPktLossEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Packet loss history result table of a MEP and remote MEP pair."
    ::= { acdCfmPacketLoss 3 }

acdCfmHistResultPktLossEntry OBJECT-TYPE
    SYNTAX      AcdCfmHistResultPktLossEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of Packet loss history result for a specific
        MEP and remote MEP pair."
    INDEX   { acdCfmHistResultPktLossID,
              acdCfmHistResultPktLossSampleIndex }
    ::=  { acdCfmHistResultPktLossTable 1 }

AcdCfmHistResultPktLossEntry ::= SEQUENCE {
    acdCfmHistResultPktLossID                   Unsigned32,
    acdCfmHistResultPktLossSampleIndex          Unsigned32,
    acdCfmHistResultPktLossStatus               INTEGER,
    acdCfmHistResultPktLossDuration             Unsigned32,
    acdCfmHistResultPktLossIntervalEnd          DateAndTime,
    acdCfmHistResultPktLossSamples              Counter32,
    acdCfmHistResultPktLossOverflowSamples      Counter32,
    acdCfmHistResultPktLossHCSamples            Counter64,
    acdCfmHistResultPktLossNbrLoss              Counter32,
    acdCfmHistResultPktLossOverflowNbrLoss      Counter32,
    acdCfmHistResultPktLossHCNbrLoss            Counter64,
    acdCfmHistResultPktLossNbrGaps              Counter32,
    acdCfmHistResultPktLossOverflowNbrGaps      Counter32,
    acdCfmHistResultPktLossHCNbrGaps            Counter64,
    acdCfmHistResultPktLossLargestGap           Counter32,
    acdCfmHistResultPktLossOverflowLargestGap   Counter32,
    acdCfmHistResultPktLossHCLargestGap         Counter64,
    acdCfmHistResultPktLossRatio                Unsigned32,
    acdCfmHistResultPktLossName                 DisplayString
}

acdCfmHistResultPktLossID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each Delay variation Measurement instance. This
        value follows the ordering of the Dm table."
    ::= { acdCfmHistResultPktLossEntry 1 }

acdCfmHistResultPktLossSampleIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same PL instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmHistResultPktLossEntry 2 }

acdCfmHistResultPktLossStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    valid(1),
                    invalid(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the validity of the packet loss results during this
        sampling interval."
    ::= { acdCfmHistResultPktLossEntry 3 }

acdCfmHistResultPktLossDuration  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interval in seconds over which the data is sampled for this entry."
    ::= { acdCfmHistResultPktLossEntry 4 }


acdCfmHistResultPktLossIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of this entry."
    ::= { acdCfmHistResultPktLossEntry 5 }

acdCfmHistResultPktLossSamples  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate packet loss results.  This is a 32 bits counter.
         Combined with the overflow counter it provides the equivalent of the
         64 bits counter acdCfmHistResultPktLossHCSamples."
    ::= { acdCfmHistResultPktLossEntry 6 }

acdCfmHistResultPktLossOverflowSamples  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmHistResultPktLossSamples
         counter has overflowed during this sampling interval. This is a
         32 bits counter. Combined with acdCfmHistResultPktLossSamples, it
         provides the equivalent of the 64 bits counter
         acdCfmHistResultPktLossHCSamples."
    ::= { acdCfmHistResultPktLossEntry 7 }

acdCfmHistResultPktLossHCSamples  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of samples gathered during the sampling
         interval to calculate packet loss results."
    ::= { acdCfmHistResultPktLossEntry 8 }

acdCfmHistResultPktLossNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets loss during this sampling interval. This is
         a 32 bits counter. Combined with the overflow counter it provides the
         equivalent of the 64 bits counter acdCfmHistResultPktLossHCNbrLoss."
    ::= { acdCfmHistResultPktLossEntry 9 }

acdCfmHistResultPktLossOverflowNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmHistResultPktLossNbrLoss counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmHistResultPktLossNbrLoss, it provides the equivalent of
         the 64 bits counter acdCfmHistResultPktLossHCNbrLoss."
    ::= { acdCfmHistResultPktLossEntry 10 }

acdCfmHistResultPktLossHCNbrLoss  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of packets loss during this sampling interval."
    ::= { acdCfmHistResultPktLossEntry 11 }

acdCfmHistResultPktLossNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of gap during this sampling interval. This is a
         32 bits counter. Combined with the overflow counter it provides the
         equivalent of the 64 bits counter acdCfmHistResultPktLossHCNbrGaps."
    ::= { acdCfmHistResultPktLossEntry 12 }

acdCfmHistResultPktLossOverflowNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmHistResultPktLossNbrGaps counter
         has overflowed during this sampling interval. This is a 32 bits counter.
         Combined with acdCfmHistResultPktLossNbrGaps, it provides the equivalent of
         the 64 bits counter acdCfmHistResultPktLossHCNbrGaps."
    ::= { acdCfmHistResultPktLossEntry 13 }

acdCfmHistResultPktLossHCNbrGaps  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of gap during this sampling interval."
    ::= { acdCfmHistResultPktLossEntry 14 }

acdCfmHistResultPktLossLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "the largest gap size in packets during this sampling interval. This is
         a 32 bits counter. Combined with the overflow counter it provides the
         equivalent of the 64 bits counter acdCfmHistResultPktLossHCNbrGaps."
    ::= { acdCfmHistResultPktLossEntry 15 }

acdCfmHistResultPktLossOverflowLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the associated acdCfmHistResultPktLossLargestGap
         counter has overflowed during this sampling interval. This is a
         32 bits counter. Combined with acdCfmHistResultPktLossLargestGap, it
         provides the equivalent of the 64 bits counter
         acdCfmHistResultPktLossHCLargestGap."
    ::= { acdCfmHistResultPktLossEntry 16 }

acdCfmHistResultPktLossHCLargestGap  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "the largest gap size in packets during this sampling interval."
    ::= { acdCfmHistResultPktLossEntry 17 }

acdCfmHistResultPktLossRatio  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the packet loss ratio. The packet loss ratio is the percent
         of packets transmitted but not received in millionth of a percent
         (1,000,000 is 1%)."
    ::= { acdCfmHistResultPktLossEntry 18 }

acdCfmHistResultPktLossName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique name used to identify this instance. The length includes the terminating NULL character."
    ::= { acdCfmHistResultPktLossEntry 19 }

---------------------------------------------------------------------------
 -- The SLM configuration table
 -- This table contains all SLM entry configurations.
---------------------------------------------------------------------------

acdCfmSlmCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmSlmCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of all SLM entries."
    ::= { acdCfmSlm 1 }

acdCfmSlmCfgEntry OBJECT-TYPE
    SYNTAX      AcdCfmSlmCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all settings to manage a SLM instance."
    INDEX   { acdCfmSlmCfgID }
    ::=  { acdCfmSlmCfgTable 1 }


AcdCfmSlmCfgEntry ::= SEQUENCE {
    acdCfmSlmCfgID              Unsigned32,
    acdCfmSlmCfgRowStatus       RowStatus,
    acdCfmSlmCfgMepIdx          Unsigned32,
    acdCfmSlmCfgRemoteMepId     Unsigned32,
    acdCfmSlmCfgPriority        Unsigned32,
    acdCfmSlmCfgState           TruthValue,
    acdCfmSlmCfgInterval        Unsigned32,
    acdCfmSlmCfgRefPeriod       Unsigned32,
    acdCfmSlmCfgNearEndThresh   Unsigned32,
    acdCfmSlmCfgFarEndThresh    Unsigned32,
    acdCfmSlmCfgName            DisplayString
}

acdCfmSlmCfgID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each SLM instance. This value follows the
         ordering the results table."
    ::= { acdCfmSlmCfgEntry 1 }

acdCfmSlmCfgRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The writable columns in a row can not be changed if the row is active.
       All columns must have a valid value before a row can be activated."
    ::= { acdCfmSlmCfgEntry 2 }

acdCfmSlmCfgMepIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maintenance association End Point Identifier."
    ::= { acdCfmSlmCfgEntry 3 }

acdCfmSlmCfgRemoteMepId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote Maintenance association End Point Identifier."
    ::= { acdCfmSlmCfgEntry 4 }

acdCfmSlmCfgPriority  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The VLAN priority. Its value ranges from 0 to 7."
     DEFVAL      { 0 }
    ::= { acdCfmSlmCfgEntry 5 }

acdCfmSlmCfgState  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "State of the SLM instance"
     DEFVAL      { false }
    ::= { acdCfmSlmCfgEntry 6 }

acdCfmSlmCfgInterval  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..10000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Interval in milliseconds at which CFM issues Synthetic Loss Measurement
        packets."
     DEFVAL      { 1000 }
    ::= { acdCfmSlmCfgEntry 7 }

acdCfmSlmCfgRefPeriod  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..1440)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reference period in minutes for Synthetic Loss Measurement."
     DEFVAL      { 15 }
    ::= { acdCfmSlmCfgEntry 8 }

acdCfmSlmCfgNearEndThresh  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Near end packet loss ratio threshold allowed without issuing an alarm
         expressed in millionth of percent (1,000,000 is 1%)."
     DEFVAL      { 1 }
    ::= { acdCfmSlmCfgEntry 9 }

acdCfmSlmCfgFarEndThresh  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Far end packet loss ratio threshold allowed without issuing an alarm
         expressed in millionth of percent (1,000,000 is 1%)."
     DEFVAL      { 0 }
    ::= { acdCfmSlmCfgEntry 10 }

acdCfmSlmCfgName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the instance"
     DEFVAL      { "new" }
    ::= { acdCfmSlmCfgEntry 11 }

---------------------------------------------------------------------------
 -- The SLM Results table
 -- This table contains all SLM results.
---------------------------------------------------------------------------

acdCfmSlmResultTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmSlmResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "SLM result table of a MEP and remote MEP pair."
    ::= { acdCfmSlm 2 }

acdCfmSlmResultEntry OBJECT-TYPE
    SYNTAX      AcdCfmSlmResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of SLM result for a specific MEP and
        remote MEP pair."
    INDEX   { acdCfmSlmResultID }
    ::=  { acdCfmSlmResultTable 1 }

AcdCfmSlmResultEntry ::= SEQUENCE {
    acdCfmSlmResultID                   Unsigned32,
    acdCfmSlmResultPeriodIndex          Unsigned32,
    acdCfmSlmResultIntervalStart        DateAndTime,
    acdCfmSlmResultValid                TruthValue,
    acdCfmSlmResultNearEndAlert         TruthValue,
    acdCfmSlmResultFarEndAlert          TruthValue,
    acdCfmSlmResultTxSlm                Counter32,
    acdCfmSlmResultRxSlr                Counter32,
    acdCfmSlmResultRemoteRxSlm          Counter32,
    acdCfmSlmResultNearEndNbrLoss       Counter32,
    acdCfmSlmResultFarEndNbrLoss        Counter32,
    acdCfmSlmResultNearEndRatio           Gauge32,
    acdCfmSlmResultFarEndRatio            Gauge32,
    acdCfmSlmResultNbrGaps              Counter32,
    acdCfmSlmResultLargestGap           Counter32,
    acdCfmSlmResultName                 DisplayString
}

acdCfmSlmResultID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each SLM instance. This
        value follows the ordering of the SLM table."
    ::= { acdCfmSlmResultEntry 1 }

acdCfmSlmResultPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same PL instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmSlmResultEntry 2 }

acdCfmSlmResultIntervalStart  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the start of the period."
    ::= { acdCfmSlmResultEntry 3 }

acdCfmSlmResultValid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reserved for future use."
    ::= { acdCfmSlmResultEntry 4 }

acdCfmSlmResultNearEndAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the SLM near end alert."
    ::= { acdCfmSlmResultEntry 5 }

acdCfmSlmResultFarEndAlert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the presence of the SLM far end alert."
    ::= { acdCfmSlmResultEntry 6 }

acdCfmSlmResultTxSlm  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLM frames sent."
    ::= { acdCfmSlmResultEntry 7 }

acdCfmSlmResultRxSlr  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLR frames received."
    ::= { acdCfmSlmResultEntry 8 }

acdCfmSlmResultRemoteRxSlm  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLM frames received at the far end."
    ::= { acdCfmSlmResultEntry 9 }

acdCfmSlmResultNearEndNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of packets lost at the near end."
    ::= { acdCfmSlmResultEntry 10 }

acdCfmSlmResultFarEndNbrLoss  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of packets lost at the far end."
    ::= { acdCfmSlmResultEntry 11 }

acdCfmSlmResultNearEndRatio  OBJECT-TYPE
    SYNTAX      Gauge32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the packet loss ratio at the near end.
        Indicates the availability ratio in millionth of a percent
        (1,000,000 is 1%)."
    ::= { acdCfmSlmResultEntry 12 }

acdCfmSlmResultFarEndRatio  OBJECT-TYPE
    SYNTAX      Gauge32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the packet loss ratio at the far end.
        Indicates the availability ratio in millionth of a percent
        (1,000,000 is 1%)."
    ::= { acdCfmSlmResultEntry 13 }

acdCfmSlmResultNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of gap."
    ::= { acdCfmSlmResultEntry 14 }

acdCfmSlmResultLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the largest gap."
    ::= { acdCfmSlmResultEntry 15 }

acdCfmSlmResultName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each SLM instance. The length includes the terminating 
         NULL character. This is a duplicate of acdCfmSlmCfgName"
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmSlmResultEntry 16 }

---------------------------------------------------------------------------
 -- The SLM History Results table
 -- This table contains all CFM Packet Loss History results.
---------------------------------------------------------------------------

acdCfmSlmHistResultTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmSlmHistResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "SLM history result table of a MEP and remote MEP pair."
    ::= { acdCfmSlm 3 }

acdCfmSlmHistResultEntry OBJECT-TYPE
    SYNTAX      AcdCfmSlmHistResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of SLM  history result for a specific
        MEP and remote MEP pair."
    INDEX   { acdCfmSlmHistResultID, acdCfmSlmHistResultPeriodIndex }
    ::=  { acdCfmSlmHistResultTable 1 }

AcdCfmSlmHistResultEntry ::= SEQUENCE {
    acdCfmSlmHistResultID                   Unsigned32,
    acdCfmSlmHistResultPeriodIndex          Unsigned32,
    acdCfmSlmHistResultIntervalEnd          DateAndTime,
    acdCfmSlmHistResultTxSlm                Counter32,
    acdCfmSlmHistResultRxSlr                Counter32,
    acdCfmSlmHistResultRemoteRxSlm          Counter32,
    acdCfmSlmHistResultNearEndRatio           Gauge32,
    acdCfmSlmHistResultFarEndRatio            Gauge32,
    acdCfmSlmHistResultNbrGaps              Counter32,
    acdCfmSlmHistResultLargestGap           Counter32,
    acdCfmSlmHistResultInstanceIndex        Unsigned32,
    acdCfmSlmHistResultName              	DisplayString
}

acdCfmSlmHistResultID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique value for each SLM instance. This
        value follows the ordering of the SLM table."
    ::= { acdCfmSlmHistResultEntry 1 }


acdCfmSlmHistResultPeriodIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An index that uniquely identifies the particular sample this entry
         represents among all samples associated with the same PL instance.
         This index starts at 1 and increases by one as each new period."
    ::= { acdCfmSlmHistResultEntry 2 }

acdCfmSlmHistResultIntervalEnd  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the time of the end of the period."
    ::= { acdCfmSlmHistResultEntry 3 }

acdCfmSlmHistResultTxSlm  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLM frames sent."
    ::= { acdCfmSlmHistResultEntry 4 }

acdCfmSlmHistResultRxSlr  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLR frames received."
    ::= { acdCfmSlmHistResultEntry 5 }

acdCfmSlmHistResultRemoteRxSlm  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of SLM frames received at the far end."
    ::= { acdCfmSlmHistResultEntry 6 }

acdCfmSlmHistResultNearEndRatio  OBJECT-TYPE
    SYNTAX      Gauge32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the packet loss ratio at the near end.
        Indicates the availability ratio in millionth of a percent
        (1,000,000 is 1%)."
    ::= { acdCfmSlmHistResultEntry 7 }

acdCfmSlmHistResultFarEndRatio  OBJECT-TYPE
    SYNTAX      Gauge32 (0..100000000)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the packet loss ratio at the far end.
        Indicates the availability ratio in millionth of a percent
        (1,000,000 is 1%)."
    ::= { acdCfmSlmHistResultEntry 8 }

acdCfmSlmHistResultNbrGaps  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the number of gap."
    ::= { acdCfmSlmHistResultEntry 9 }

acdCfmSlmHistResultLargestGap  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the largest gap."
    ::= { acdCfmSlmHistResultEntry 10 }

acdCfmSlmHistResultInstanceIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The instance index."
    ::= { acdCfmSlmHistResultEntry 11 }

acdCfmSlmHistResultName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each SLM instance. The length includes the terminating 
         NULL character. This is a duplicate of acdCfmSlmCfgName"
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmSlmHistResultEntry 12 }

---------------------------------------------------------------------------
 -- The MEP Transmit Statistics table
 -- This table contains all transmit statistics related to all MEP entries.
---------------------------------------------------------------------------

acdCfmMepStatsTxTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmMepStatsTxEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Transmit Statictics table of all MEP entries."
    ::= { acdCfmMep 2 }

acdCfmMepStatsTxEntry OBJECT-TYPE
    SYNTAX      AcdCfmMepStatsTxEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all transmit statistics related to a MEP entry."
    INDEX   { acdCfmMepStatsTxID }
    ::=  { acdCfmMepStatsTxTable 1 }

AcdCfmMepStatsTxEntry ::= SEQUENCE {
    acdCfmMepStatsTxID                      Unsigned32,
    acdCfmMepStatsTxCcmPdu                  Counter64,
    acdCfmMepStatsTxLbmPdu                  Counter64,
    acdCfmMepStatsTxLbrPdu                  Counter64,
    acdCfmMepStatsTxLtmPdu                  Counter64,
    acdCfmMepStatsTxLtrPdu                  Counter64,
    acdCfmMepStatsTxAisPdu                  Counter64,
    acdCfmMepStatsTxLckPdu                  Counter64,
    acdCfmMepStatsTxTstPdu                  Counter64,
    acdCfmMepStatsTxLinearApsPdu            Counter64,
    acdCfmMepStatsTxRingApsPdu              Counter64,
    acdCfmMepStatsTxMccPdu                  Counter64,
    acdCfmMepStatsTxLmmPdu                  Counter64,
    acdCfmMepStatsTxLmrPdu                  Counter64,
    acdCfmMepStatsTx1dmPdu                  Counter64,
    acdCfmMepStatsTxDmmPdu                  Counter64,
    acdCfmMepStatsTxDmrPdu                  Counter64,
    acdCfmMepStatsTxExmPdu                  Counter64,
    acdCfmMepStatsTxExrPdu                  Counter64,
    acdCfmMepStatsTxVsmPdu                  Counter64,
    acdCfmMepStatsTxVsrPdu                  Counter64,
    acdCfmMepStatsTxCsfPdu                  Counter64,
    acdCfmMepStatsTxSlmPdu                  Counter64,
    acdCfmMepStatsTxSlrPdu                  Counter64,
    acdCfmMepStatsTxName                    DisplayString

}

acdCfmMepStatsTxID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Unique value for each MEP instance. This value follows the ordering
        of the MEP table."
    ::= { acdCfmMepStatsTxEntry 1 }

acdCfmMepStatsTxCcmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Continuity Check Message (CCM)
         PDU transmitted by the MEP (OpCode 1)."
    ::= { acdCfmMepStatsTxEntry 2 }

acdCfmMepStatsTxLbmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of LoopBack Message (LBM)
         PDU transmitted by the MEP (OpCode 3)."
    ::= { acdCfmMepStatsTxEntry 3 }

acdCfmMepStatsTxLbrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of LoopBack Reply (LBR)
         PDU transmitted by the MEP (OpCode 2)."
    ::= { acdCfmMepStatsTxEntry 4 }

acdCfmMepStatsTxLtmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Link Trace Message (LTM)
         PDU transmitted by the MEP (OpCode 5)."
    ::= { acdCfmMepStatsTxEntry 5 }

acdCfmMepStatsTxLtrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Link Trace Reply (LTR)
         PDU transmitted by the MEP (OpCode 4)."
    ::= { acdCfmMepStatsTxEntry 6 }

acdCfmMepStatsTxAisPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Alarm Indication Signal (AIS)
         PDU transmitted by the MEP (OpCode 33)."
    ::= { acdCfmMepStatsTxEntry 7 }

acdCfmMepStatsTxLckPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Locked (LCK) PDU transmitted
         by the MEP  (OpCode 35)."
    ::= { acdCfmMepStatsTxEntry 8 }

acdCfmMepStatsTxTstPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Test (TST) PDU transmitted by
         the MEP (OpCode 37)."
    ::= { acdCfmMepStatsTxEntry 9 }

acdCfmMepStatsTxLinearApsPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of linear Automatic Protection Switching
         (APS) PDU transmitted by the MEP  (OpCode 39)."
    ::= { acdCfmMepStatsTxEntry 10 }

acdCfmMepStatsTxRingApsPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of ring Automatic Protection Switching
         (APS) PDU transmitted by the MEP (OpCode 40)."
    ::= { acdCfmMepStatsTxEntry 11 }

acdCfmMepStatsTxMccPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Maintenance Communication
         Channel  (MCC) PDU transmitted by the MEP (OpCode 41)."
    ::= { acdCfmMepStatsTxEntry 12 }

acdCfmMepStatsTxLmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Loss Measurement Message (LMM)
         PDU transmitted by the MEP (OpCode 43)."
    ::= { acdCfmMepStatsTxEntry 13 }

acdCfmMepStatsTxLmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Loss Measurement Reply (LMR)
         PDU transmitted by the MEP (OpCode 42)."
    ::= { acdCfmMepStatsTxEntry 14 }

acdCfmMepStatsTx1dmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of One-way Delay Measurement (1DM)
         PDU transmitted by the MEP (OpCode 45)."
    ::= { acdCfmMepStatsTxEntry 15 }

acdCfmMepStatsTxDmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Message (DMM)
         PDU transmitted by the MEP (OpCode 47)."
    ::= { acdCfmMepStatsTxEntry 16 }

acdCfmMepStatsTxDmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Reply (DMR)
         PDU transmitted by the MEP (OpCode 46)."
    ::= { acdCfmMepStatsTxEntry 17 }

acdCfmMepStatsTxExmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of EXperimental Message (EXM)
         PDU transmitted by the MEP (OpCode 49)."
    ::= { acdCfmMepStatsTxEntry 18 }

acdCfmMepStatsTxExrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of EXperimental Reply (EXR)
         PDU transmitted by the MEP (OpCode 48)."
    ::= { acdCfmMepStatsTxEntry 19 }

acdCfmMepStatsTxVsmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Vendor Specific Message (VSM)
         PDU transmitted by the MEP  (OpCode 51)."
    ::= { acdCfmMepStatsTxEntry 20 }

acdCfmMepStatsTxVsrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Vendor Specific Reply (VSR)
         PDU transmitted by the MEP (OpCode 50)."
    ::= { acdCfmMepStatsTxEntry 21 }

acdCfmMepStatsTxCsfPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Client Signal Fail (CSF)
         PDU transmitted by the MEP (OpCode 52)."
    ::= { acdCfmMepStatsTxEntry 22 }

acdCfmMepStatsTxSlmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Synthetic Loss Message (SLM)
         PDU transmitted by the MEP (OpCode 55)."
    ::= { acdCfmMepStatsTxEntry 23 }

acdCfmMepStatsTxSlrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Synthetic Loss Reply (SLR)
         PDU transmitted by the MEP (OpCode 54)."
    ::= { acdCfmMepStatsTxEntry 24 }

acdCfmMepStatsTxName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each Mep instance. The length includes the terminating 
         NULL character. This is a duplicate of acdCfmMepCfgName"
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmMepStatsTxEntry 25 }



---------------------------------------------------------------------------
 -- The MEP Receive Statistics table
 -- This table contains all receive statistics related to all MEP entries.
---------------------------------------------------------------------------

acdCfmMepStatsRxTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmMepStatsRxEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Receive Statictics table of all MEP entries."
    ::= { acdCfmMep 3 }

acdCfmMepStatsRxEntry OBJECT-TYPE
    SYNTAX      AcdCfmMepStatsRxEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all receive statistics related to a MEP entry."
    INDEX   { acdCfmMepStatsRxID }
    ::=  { acdCfmMepStatsRxTable 1 }

AcdCfmMepStatsRxEntry ::= SEQUENCE {
    acdCfmMepStatsRxID                      Unsigned32,
    acdCfmMepStatsRxCcmPdu                  Counter64,
    acdCfmMepStatsRxLbmPdu                  Counter64,
    acdCfmMepStatsRxLbrPdu                  Counter64,
    acdCfmMepStatsRxLtmPdu                  Counter64,
    acdCfmMepStatsRxLtrPdu                  Counter64,
    acdCfmMepStatsRxAisPdu                  Counter64,
    acdCfmMepStatsRxLckPdu                  Counter64,
    acdCfmMepStatsRxTstPdu                  Counter64,
    acdCfmMepStatsRxLinearApsPdu            Counter64,
    acdCfmMepStatsRxRingApsPdu              Counter64,
    acdCfmMepStatsRxMccPdu                  Counter64,
    acdCfmMepStatsRxLmmPdu                  Counter64,
    acdCfmMepStatsRxLmrPdu                  Counter64,
    acdCfmMepStatsRx1dmPdu                  Counter64,
    acdCfmMepStatsRxDmmPdu                  Counter64,
    acdCfmMepStatsRxDmrPdu                  Counter64,
    acdCfmMepStatsRxExmPdu                  Counter64,
    acdCfmMepStatsRxExrPdu                  Counter64,
    acdCfmMepStatsRxVsmPdu                  Counter64,
    acdCfmMepStatsRxVsrPdu                  Counter64,

    acdCfmMepStatsRxCcmSeqErrors            Counter64,
    acdCfmMepStatsRxLtrUnexpectedPdu        Counter64,
    acdCfmMepStatsRxLtrMacErrors            Counter64,
    acdCfmMepStatsRxLbrOooErrors            Counter64,
    acdCfmMepStatsRxLbrUnexpectedPdu        Counter64,
    acdCfmMepStatsRxLbrDataErrors           Counter64,
    acdCfmMepStatsRxCsfPdu                  Counter64,
    acdCfmMepStatsRxSlmPdu                  Counter64,
    acdCfmMepStatsRxSlrPdu                  Counter64,
    acdCfmMepStatsRxCsfInvalidFlags         Counter64,
    acdCfmMepStatsRxName                    DisplayString

}

acdCfmMepStatsRxID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "."
    ::= { acdCfmMepStatsRxEntry 1 }

acdCfmMepStatsRxCcmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Continuity Check Message (CCM)
         PDU received by the MEP  (OpCode 1)."
    ::= { acdCfmMepStatsRxEntry 2 }

acdCfmMepStatsRxLbmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of LoopBack Message (LBM)
         PDU received by the MEP  (OpCode 3)."
    ::= { acdCfmMepStatsRxEntry 3 }

acdCfmMepStatsRxLbrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of LoopBack Reply (LBR)
         PDU received by the MEP  (OpCode 2)."
    ::= { acdCfmMepStatsRxEntry 4 }

acdCfmMepStatsRxLtmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Link Trace Message (LTM)
         PDU received by the MEP  (OpCode 5)."
    ::= { acdCfmMepStatsRxEntry 5 }

acdCfmMepStatsRxLtrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Link Trace Reply (LTR)
         PDU received by the MEP  (OpCode 4)."
    ::= { acdCfmMepStatsRxEntry 6 }

acdCfmMepStatsRxAisPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Alarm Indication Signal (AIS)
         PDU received by the MEP  (OpCode 33)."
    ::= { acdCfmMepStatsRxEntry 7 }

acdCfmMepStatsRxLckPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Locked (LCK) PDU received
         by the MEP  (OpCode 35)."
    ::= { acdCfmMepStatsRxEntry 8 }

acdCfmMepStatsRxTstPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Test (TST) PDU received by
         the MEP  (OpCode 37)."
    ::= { acdCfmMepStatsRxEntry 9 }

acdCfmMepStatsRxLinearApsPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of linear Automatic Protection Switching
         (APS) PDU received by the MEP (OpCode 39)."
    ::= { acdCfmMepStatsRxEntry 10 }

acdCfmMepStatsRxRingApsPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of ring Automatic Protection Switching
         (APS) PDU received by the MEP (OpCode 40)."
    ::= { acdCfmMepStatsRxEntry 11 }

acdCfmMepStatsRxMccPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Maintenance Communication
         Channel (MCC) PDU received by the MEP (OpCode 41)."
    ::= { acdCfmMepStatsRxEntry 12 }

acdCfmMepStatsRxLmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Loss Measurement Message (LMM)
         PDU received by the MEP (OpCode 43)."
    ::= { acdCfmMepStatsRxEntry 13 }

acdCfmMepStatsRxLmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Loss Measurement Reply (LMR)
         PDU received by the MEP  (OpCode 42)."
    ::= { acdCfmMepStatsRxEntry 14 }

acdCfmMepStatsRx1dmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of One-way Delay Measurement (1DM)
         PDU received by the MEP (OpCode 45)."
    ::= { acdCfmMepStatsRxEntry 15 }

acdCfmMepStatsRxDmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Message (DMM)
         PDU received by the MEP (OpCode 47)."
    ::= { acdCfmMepStatsRxEntry 16 }

acdCfmMepStatsRxDmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Reply (DMR)
         PDU received by the MEP (OpCode 46)."
    ::= { acdCfmMepStatsRxEntry 17 }

acdCfmMepStatsRxExmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of EXperimental Message (EXM)
         PDU received by the MEP (OpCode 49)."
    ::= { acdCfmMepStatsRxEntry 18 }

acdCfmMepStatsRxExrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of EXperimental Reply (EXR)
         PDU received by the MEP (OpCode 48)."
    ::= { acdCfmMepStatsRxEntry 19 }

acdCfmMepStatsRxVsmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Vendor Specific Message (VSM)
         PDU received by the MEP (OpCode 51)."
    ::= { acdCfmMepStatsRxEntry 20 }

acdCfmMepStatsRxVsrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Vendor Specific Reply (VSR)
         PDU received by the MEP (OpCode 50)."
    ::= { acdCfmMepStatsRxEntry 21 }

    acdCfmMepStatsRxCcmSeqErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of out-of-sequence CCMs received from all remote
         MEPs."
    ::= { acdCfmMepStatsRxEntry 22 }

    acdCfmMepStatsRxLtrUnexpectedPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of LTRs received when no linktrace request is active
         for that MEP."
    ::= { acdCfmMepStatsRxEntry 23 }

    acdCfmMepStatsRxLtrMacErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Link Trace Replies dropped because of bad MAC
         address."
    ::= { acdCfmMepStatsRxEntry 24 }

    acdCfmMepStatsRxLbrOooErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of valid, out-of-order Loopback Replies received."
    ::= { acdCfmMepStatsRxEntry 25 }

    acdCfmMepStatsRxLbrUnexpectedPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of LBRs received when no loopback request is active
         for that MEP."
    ::= { acdCfmMepStatsRxEntry 26 }

    acdCfmMepStatsRxLbrDataErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of LBRs received whose MACService Data Unit did not
          match (except for the OpCode) that of the corresponding LBM."
    ::= { acdCfmMepStatsRxEntry 27 }

acdCfmMepStatsRxCsfPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Client Signal Fail (CSF)
         PDU received by the MEP (OpCode 52)."
    ::= { acdCfmMepStatsRxEntry 28 }

acdCfmMepStatsRxSlmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Synthetic Loss Message (SLM)
         PDU received by the MEP (OpCode 55)."
    ::= { acdCfmMepStatsRxEntry 29 }

acdCfmMepStatsRxSlrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Synthetic Loss Reply (SLR)
         PDU received by the MEP (OpCode 54)."
    ::= { acdCfmMepStatsRxEntry 30 }

acdCfmMepStatsRxCsfInvalidFlags  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of ETH-CSF PDUs received with
         invalid flags."
    ::= { acdCfmMepStatsRxEntry 31 }

acdCfmMepStatsRxName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each Mep instance. The length includes the terminating 
         NULL character. This is a duplicate of acdCfmMepCfgName"
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmMepStatsRxEntry 32 }



---------------------------------------------------------------------------
 -- The DMM/DMR Statistics table
 -- This table contains all DMM/DMR statistics related to a MEP entry.
---------------------------------------------------------------------------

acdCfmMepDmStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmMepDmStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Transmit DMM/DMR statictics per priority table for a MEP entry."
    ::= { acdCfmMep 4 }

acdCfmMepDmStatsEntry OBJECT-TYPE
    SYNTAX      AcdCfmMepDmStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all DMM/DMR statistics related to a MEP entry."
    INDEX   { acdCfmMepDmStatsID, acdCfmMepDmStatsPriority }
    ::=  { acdCfmMepDmStatsTable 1 }

AcdCfmMepDmStatsEntry ::= SEQUENCE {
    acdCfmMepDmStatsID                      Unsigned32,
    acdCfmMepDmStatsPriority                Unsigned32,
    acdCfmMepDmStatsTxDmmPdu                Counter64,
    acdCfmMepDmStatsRxDmmPdu                Counter64,
    acdCfmMepDmStatsTxDmrPdu                Counter64,
    acdCfmMepDmStatsRxDmrPdu                Counter64,
    acdCfmMepDmStatsName                    DisplayString
}

acdCfmMepDmStatsID  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Unique value for each MEP instance. This value follows the ordering
        of the MEP table. Same as acdCfmMepStatsTxID and acdCfmMepStatsRxID."
    ::= { acdCfmMepDmStatsEntry 1 }

acdCfmMepDmStatsPriority  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Unique value for each priority level."
    ::= { acdCfmMepDmStatsEntry 2 }

acdCfmMepDmStatsTxDmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Message (DMM)
         (OpCode 47) PDU transmitted by the MEP for this specific priority level."
    ::= { acdCfmMepDmStatsEntry 3 }

acdCfmMepDmStatsRxDmmPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Message (DMM)
         (OpCode 47) PDU received by the MEP for this specific priority level."
    ::= { acdCfmMepDmStatsEntry 4 }

acdCfmMepDmStatsTxDmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Reply (DMR)
         (OpCode 46) PDU transmitted by the MEP for this specific priority level."
    ::= { acdCfmMepDmStatsEntry 5 }

acdCfmMepDmStatsRxDmrPdu  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is a count of the total number of Delay Measurement Reply (DMR)
         (OpCode 46) PDU received by the MEP for this specific priority level."
    ::= { acdCfmMepDmStatsEntry 6 }

acdCfmMepDmStatsName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unique string for each Mep instance. The length includes the terminating 
         NULL character. This is a duplicate of acdCfmMepCfgName"
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmMepDmStatsEntry 7 }

---------------------------------------------------------------------------
 -- The MEP configuration table
 -- This table contains all MEP entry configurations.
---------------------------------------------------------------------------

acdCfmMepCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmMepCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of all MEP entries."
    ::= { acdCfmMep 5 }

acdCfmMepCfgEntry OBJECT-TYPE
    SYNTAX      AcdCfmMepCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all settings to manage a MEP instance."
    INDEX   { acdCfmMepCfgIdx }
    ::=  { acdCfmMepCfgTable 1 }


AcdCfmMepCfgEntry ::= SEQUENCE {
    acdCfmMepCfgIdx                       Unsigned32,
    acdCfmMepCfgRowStatus                 RowStatus,
    acdCfmMepCfgMdIdx                     Unsigned32,
    acdCfmMepCfgMaIdx                     Unsigned32,
    acdCfmMepCfgMepId                     Unsigned32,
    acdCfmMepCfgName                      DisplayString,
    acdCfmMepCfgPortId                    Unsigned32,
    acdCfmMepCfgPortIdMacAddr             MacAddress,
    acdCfmMepCfgDirection                 AcdCfmMepDirection,
    acdCfmMepCfgPrimaryVid                VlanIdOrNone,
    acdCfmMepCfgActive                    TruthValue,
    acdCfmMepCfgCciEnable                 TruthValue,
    acdCfmMepCfgCcmSeqEnable              TruthValue,
    acdCfmMepCfgPriority                  Unsigned32,
    acdCfmMepCfgAlarmPri                  AcdCfmMepLowestAlarmPri,
    acdCfmMepCfgFngAlarmTime              Unsigned32,
    acdCfmMepCfgFngResetTime              Unsigned32,
    acdCfmMepCfgFpEnable                  TruthValue,
    acdCfmMepCfgFpPortId                  Unsigned32,
    acdCfmMepCfgCsfEnable                 TruthValue,
    acdCfmMepCfgInterfaceStatusTLVEnable  TruthValue
}

acdCfmMepCfgIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Unique value for each MEP instance. This value follows the
         ordering the status table."
    ::= { acdCfmMepCfgEntry 1 }

acdCfmMepCfgRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The writable columns in a row can not be changed if the row is active.
       All columns must have a valid value before a row can be activated."
    ::= { acdCfmMepCfgEntry 2 }

acdCfmMepCfgMdIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maintenance Domain instance index."
     ::= { acdCfmMepCfgEntry 3 }

acdCfmMepCfgMaIdx  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maintenance Association instance index."
    ::= { acdCfmMepCfgEntry 4 }

acdCfmMepCfgMepId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maintenance association End Point Identifier."
    ::= { acdCfmMepCfgEntry 5 }

acdCfmMepCfgName  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Unique string for each Mep instance. The length includes the terminating NULL character."
    DEFVAL      { ''H }   -- the empty string
    ::= { acdCfmMepCfgEntry 6 }

acdCfmMepCfgPortId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Port Identifier."
     DEFVAL      { 1 }
    ::= { acdCfmMepCfgEntry 7 }

acdCfmMepCfgPortIdMacAddr  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "MAC Address of the port."
     ::= { acdCfmMepCfgEntry 8 }

acdCfmMepCfgDirection  OBJECT-TYPE
    SYNTAX      AcdCfmMepDirection
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Direction in which the Maintenance association (MEP) faces on the bridge port."
     DEFVAL      { 1 }
    ::= { acdCfmMepCfgEntry 9 }

acdCfmMepCfgPrimaryVid  OBJECT-TYPE
    SYNTAX      VlanIdOrNone
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Primary Vlan Id."
     DEFVAL      { 0 }
    ::= { acdCfmMepCfgEntry 10 }

acdCfmMepCfgActive  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Administrative state of the MEP.
        A Boolean indicating the administrative state of the MEP."
     DEFVAL      { false }
    ::= { acdCfmMepCfgEntry 11 }

acdCfmMepCfgCciEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If set to true, the MEP will generate CCM messages."
     DEFVAL      { false }
    ::= { acdCfmMepCfgEntry 12 }

acdCfmMepCfgCcmSeqEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If set to true, the sequence number in the CCM PDU will increment."
     DEFVAL      { false }
    ::= { acdCfmMepCfgEntry 13 }

acdCfmMepCfgPriority  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The priority value for CCMs and LTMs transmitted by the MEP."
    ::= { acdCfmMepCfgEntry 14 }

acdCfmMepCfgAlarmPri  OBJECT-TYPE
    SYNTAX      AcdCfmMepLowestAlarmPri
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The highest priority defect that has been present since the
        MEPs Fault Notification Generator State Machine was last in
        the FNG_RESET state."
     ::= { acdCfmMepCfgEntry 15 }

acdCfmMepCfgFngAlarmTime  OBJECT-TYPE
    SYNTAX      Unsigned32  (2500..10000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The time that defects must be present before a Fault Alarm is
        issued (default 2500 milliseconds)."
    DEFVAL { 2500 }
     ::= { acdCfmMepCfgEntry 16 }

acdCfmMepCfgFngResetTime  OBJECT-TYPE
    SYNTAX      Unsigned32  (2500..10000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The time that defects must be present before a Fault Alarm is
        issued (default 10000 milliseconds)."
    DEFVAL { 10000 }
     ::= { acdCfmMepCfgEntry 17 }

acdCfmMepCfgFpEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If set to true, the faults generated by this MEP will be propagated to the Fault Propagation port."
     DEFVAL      { false }
     ::= { acdCfmMepCfgEntry 18 }

acdCfmMepCfgFpPortId  OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The fault propagation port used to propagate faults."
     ::= { acdCfmMepCfgEntry 19 }

acdCfmMepCfgCsfEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If set to true, Client Signal Fail errors will be propagated to the Fault Propagation port."
     DEFVAL      { false }
     ::= { acdCfmMepCfgEntry 20 }

acdCfmMepCfgInterfaceStatusTLVEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If set to true, Interface Status TLV will be included in Down MEP CCM PDU. Interface status is obtained from the Fault Propagation port."
     DEFVAL      { false }
     ::= { acdCfmMepCfgEntry 21 }



---------------------------------------------------------------------------
 -- The Configuration manager Stack Table...
 -- This table ties some information together
---------------------------------------------------------------------------

acdCfmStackTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmStackEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of stack entries."
    ::= { acdCfmStack 1 }

acdCfmStackEntry OBJECT-TYPE
    SYNTAX      AcdCfmStackEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all informations to tie together."
    INDEX   { acdCfmMdIdx, acdCfmMaIdx, acdCfmMepID}
    ::=  { acdCfmStackTable 1 }

AcdCfmStackEntry ::= SEQUENCE {
    acdCfmMdIdx                            Unsigned32,
    acdCfmMaIdx                            Unsigned32,
    acdCfmMepID                            Unsigned32,
    acdCfmMepIdx                           Unsigned32
  }

acdCfmMdIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Maintenance Domain(MD) index from table dot1agCfmMepTable in IEEE8021-CFM-MIB."
    ::= { acdCfmStackEntry 1 }

acdCfmMaIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Maintenance Association(MA) index from table dot1agCfmMepTable in IEEE8021-CFM-MIB."
    ::= { acdCfmStackEntry 2 }

acdCfmMepID OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Maintenance End Point(Mep) index from table dot1agCfmMepTable in IEEE8021-CFM-MIB."
    ::= { acdCfmStackEntry 3 }

acdCfmMepIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maintenance End Point(Mep) index from table acdCfmDmCfgTable in ACD-CFM-MIB."
    ::= { acdCfmStackEntry 4 }


---------------------------------------------------------------------------
 -- The Interface Assign configuration table
 -- This table contains the Interface Assign entry configurations.
---------------------------------------------------------------------------

acdCfmCfgIfAssignTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AcdCfmCfgIfAssignEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Configuration table of interface assign entries."
    ::= { acdCfmConfig 1 }

acdCfmCfgIfAssignEntry OBJECT-TYPE
    SYNTAX      AcdCfmCfgIfAssignEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry consisting of all settings to assign/unassign an
         interface to a mep."
    INDEX   { acdCfmCfgIfAssignInstIdx }
    ::=  { acdCfmCfgIfAssignTable 1 }

AcdCfmCfgIfAssignEntry ::= SEQUENCE {
    acdCfmCfgIfAssignRowStatus                RowStatus,
    acdCfmCfgIfAssignInstIdx                  Unsigned32,
    acdCfmCfgIfAssignIfName                   DisplayString,
    acdCfmCfgIfAssignLockAssign               AcdCfmInterfaceAssign
}

acdCfmCfgIfAssignRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "All columns must have a valid value before a row can be activated."
    ::= { acdCfmCfgIfAssignEntry 1 }

acdCfmCfgIfAssignInstIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Interface ID of interface to assign/unassing. The numbering of 
         this index is non-contiguous. Interfaces not present in the
         table cannot be assigned to a mep."
    ::= { acdCfmCfgIfAssignEntry 2 }

acdCfmCfgIfAssignIfName  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "System interface name of the interface to assign/unassign."
    ::= { acdCfmCfgIfAssignEntry 3 }

acdCfmCfgIfAssignLockAssign  OBJECT-TYPE
    SYNTAX      AcdCfmInterfaceAssign
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The current lock assignment configuration on an interface."
    DEFVAL      { unassigned }
    ::= { acdCfmCfgIfAssignEntry 4 }

--------------------------------------------------------------------------
 -- ACD-CFM-MIB Module - Conformance Information
---------------------------------------------------------------------------

acdCfmCompliances   OBJECT IDENTIFIER ::= { acdCfmConformance 1 }
acdCfmGroups        OBJECT IDENTIFIER ::= { acdCfmConformance 2 }

---------------------------------------------------------------------------
 -- Units of conformance
---------------------------------------------------------------------------

acdCfmDmCfgGroup OBJECT-GROUP
    OBJECTS {
        acdCfmDmCfgRowStatus,
        acdCfmDmCfgMepIdx,
        acdCfmDmCfgRemoteMepId,
        acdCfmDmCfgPriority,
        acdCfmDmCfgEnable,
        acdCfmDmCfgInterval,
        acdCfmDmCfgRefPeriod,
        acdCfmDmCfgOneWayDelayEnable,
        acdCfmDmCfgOneWayDelayMax,
        acdCfmDmCfgOneWayDelayThresh,
        acdCfmDmCfgOneWayAvgDelayThresh,
        acdCfmDmCfgOneWayDvEnable,
        acdCfmDmCfgOneWayDvMax,
        acdCfmDmCfgOneWayDvThresh,
        acdCfmDmCfgOneWayAvgDvThresh,
        acdCfmDmCfgTwoWayDelayEnable,
        acdCfmDmCfgTwoWayDelayMax,
        acdCfmDmCfgTwoWayDelayThresh,
        acdCfmDmCfgTwoWayAvgDelayThresh,
        acdCfmDmCfgTwoWayDvEnable,
        acdCfmDmCfgTwoWayDvMax,
        acdCfmDmCfgTwoWayDvThresh,
        acdCfmDmCfgTwoWayAvgDvThresh,
        acdCfmDmCfgName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the Delay Measurement configuration Group."
    ::= { acdCfmGroups 1 }

acdCfmResultOneWayDelayGroup OBJECT-GROUP
    OBJECTS {
        acdCfmResultOneWayDelayPeriodIndex,
        acdCfmResultOneWayDelayIntervalStart,
        acdCfmResultOneWayDelayValid,
        acdCfmResultOneWayDelayAlert,
        acdCfmResultOneWayDelayAvgAlert,
        acdCfmResultOneWayDelaySamples,
        acdCfmResultOneWayDelayMinValue,
        acdCfmResultOneWayDelayMaxValue,
        acdCfmResultOneWayDelayAvgValue,
        acdCfmResultOneWayDelayThreshExc,
        acdCfmResultOneWayDelayInstValue,
        acdCfmResultOneWayDelayName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the One Way Delay result Group."
    ::= { acdCfmGroups 2 }

acdCfmResultOneWayDvGroup OBJECT-GROUP
    OBJECTS {
        acdCfmResultOneWayDvPeriodIndex,
        acdCfmResultOneWayDvIntervalStart,
        acdCfmResultOneWayDvValid,
        acdCfmResultOneWayDvAlert,
        acdCfmResultOneWayDvAvgAlert,
        acdCfmResultOneWayDvSamples,
        acdCfmResultOneWayDvMinValue,
        acdCfmResultOneWayDvMaxValue,
        acdCfmResultOneWayDvAvgValue,
        acdCfmResultOneWayDvThreshExc,
        acdCfmResultOneWayDvInstValue,
        acdCfmResultOneWayDvName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the One Way Delay variation result Group."
    ::= { acdCfmGroups 3 }

acdCfmResultTwoWayDelayGroup OBJECT-GROUP
    OBJECTS {
        acdCfmResultTwoWayDelayPeriodIndex,
        acdCfmResultTwoWayDelayIntervalStart,
        acdCfmResultTwoWayDelayValid,
        acdCfmResultTwoWayDelayAlert,
        acdCfmResultTwoWayDelayAvgAlert,
        acdCfmResultTwoWayDelaySamples,
        acdCfmResultTwoWayDelayMinValue,
        acdCfmResultTwoWayDelayMaxValue,
        acdCfmResultTwoWayDelayAvgValue,
        acdCfmResultTwoWayDelayThreshExc,
        acdCfmResultTwoWayDelayInstValue,
        acdCfmResultTwoWayDelayName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the Two Way Delay result Group."
    ::= { acdCfmGroups 4 }

acdCfmResultTwoWayDvGroup OBJECT-GROUP
    OBJECTS {
        acdCfmResultTwoWayDvPeriodIndex,
        acdCfmResultTwoWayDvIntervalStart,
        acdCfmResultTwoWayDvValid,
        acdCfmResultTwoWayDvAlert,
        acdCfmResultTwoWayDvAvgAlert,
        acdCfmResultTwoWayDvSamples,
        acdCfmResultTwoWayDvMinValue,
        acdCfmResultTwoWayDvMaxValue,
        acdCfmResultTwoWayDvAvgValue,
        acdCfmResultTwoWayDvThreshExc,
        acdCfmResultTwoWayDvInstValue,
        acdCfmResultTwoWayDvName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the Two Way Delay varition result Group."
    ::= { acdCfmGroups 5 }

acdCfmHistResultOneWayDelayGroup OBJECT-GROUP
    OBJECTS {
        acdCfmHistResultOneWayDelayID,
        acdCfmHistResultOneWayDelaySampleIndex,
        acdCfmHistResultOneWayDelayStatus,
        acdCfmHistResultOneWayDelayDuration,
        acdCfmHistResultOneWayDelayIntervalEnd,
        acdCfmHistResultOneWayDelaySamples,
        acdCfmHistResultOneWayDelayMinValue,
        acdCfmHistResultOneWayDelayMaxValue,
        acdCfmHistResultOneWayDelayAvgValue,
        acdCfmHistResultOneWayDelayThreshExc,
        acdCfmHistResultOneWayDelayName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the One Way Delay history result Group."
    ::= { acdCfmGroups 6 }

acdCfmHistResultOneWayDvGroup OBJECT-GROUP
    OBJECTS {
        acdCfmHistResultOneWayDvID,
        acdCfmHistResultOneWayDvSampleIndex,
        acdCfmHistResultOneWayDvStatus,
        acdCfmHistResultOneWayDvDuration,
        acdCfmHistResultOneWayDvIntervalEnd,
        acdCfmHistResultOneWayDvSamples,
        acdCfmHistResultOneWayDvMinValue,
        acdCfmHistResultOneWayDvMaxValue,
        acdCfmHistResultOneWayDvAvgValue,
        acdCfmHistResultOneWayDvThreshExc,
        acdCfmHistResultOneWayDvName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the One Way Delay variation history result Group."
    ::= { acdCfmGroups 7 }

acdCfmHistResultTwoWayDelayGroup OBJECT-GROUP
    OBJECTS {
        acdCfmHistResultTwoWayDelayID,
        acdCfmHistResultTwoWayDelaySampleIndex,
        acdCfmHistResultTwoWayDelayStatus,
        acdCfmHistResultTwoWayDelayDuration,
        acdCfmHistResultTwoWayDelayIntervalEnd,
        acdCfmHistResultTwoWayDelaySamples,
        acdCfmHistResultTwoWayDelayMinValue,
        acdCfmHistResultTwoWayDelayMaxValue,
        acdCfmHistResultTwoWayDelayAvgValue,
        acdCfmHistResultTwoWayDelayThreshExc,
        acdCfmHistResultTwoWayDelayName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the Two Way Delay history result Group."
    ::= { acdCfmGroups 8 }

acdCfmHistResultTwoWayDvGroup OBJECT-GROUP
    OBJECTS {
        acdCfmHistResultTwoWayDvID,
        acdCfmHistResultTwoWayDvSampleIndex,
        acdCfmHistResultTwoWayDvStatus,
        acdCfmHistResultTwoWayDvDuration,
        acdCfmHistResultTwoWayDvIntervalEnd,
        acdCfmHistResultTwoWayDvSamples,
        acdCfmHistResultTwoWayDvMinValue,
        acdCfmHistResultTwoWayDvMaxValue,
        acdCfmHistResultTwoWayDvAvgValue,
        acdCfmHistResultTwoWayDvThreshExc,
        acdCfmHistResultTwoWayDvName
    }
    STATUS      current
    DESCRIPTION
       "Objects for the Two Way Delay variation history result Group."
    ::= { acdCfmGroups 9 }


acdCfmPktLossCfgGroup OBJECT-GROUP
    OBJECTS {
        acdCfmPktLossCfgRowStatus,
        acdCfmPktLossCfgMepIdx,
        acdCfmPktLossCfgRemoteMepId,
        acdCfmPktLossCfgPriority,
        acdCfmPktLossCfgEnable,
        acdCfmPktLossCfgInterval,
        acdCfmPktLossCfgRefPeriod,
        acdCfmPktLossCfgThresh,
        acdCfmPktLossCfgRatioThresh,
	acdCfmPktLossCfgName
    }
    STATUS      current
    DESCRIPTION
       "Objects for Packet loss configuration Group."
    ::= { acdCfmGroups 10 }

acdCfmResultPktLossGroup OBJECT-GROUP
    OBJECTS {
        acdCfmResultPktLossPeriodIndex,
        acdCfmResultPktLossIntervalStart,
        acdCfmResultPktLossValid,
        acdCfmResultPktLossAlert,
        acdCfmResultPktLossSamples,
        acdCfmResultPktLossOverflowSamples,
        acdCfmResultPktLossHCSamples,
        acdCfmResultPktLossNbrLoss,
        acdCfmResultPktLossOverflowNbrLoss,
        acdCfmResultPktLossHCNbrLoss,
        acdCfmResultPktLossNbrGaps,
        acdCfmResultPktLossOverflowNbrGaps,
        acdCfmResultPktLossHCNbrGaps,
        acdCfmResultPktLossLargestGap,
        acdCfmResultPktLossOverflowLargestGap,
        acdCfmResultPktLossHCLargestGap,
        acdCfmResultPktLossRatio,
        acdCfmResultPktLossName
    }
    STATUS      current
    DESCRIPTION
       "Objects for Packet loss result Group."
    ::= { acdCfmGroups 11 }

acdCfmHistResultPktLossGroup OBJECT-GROUP
    OBJECTS {
        acdCfmHistResultPktLossID,
        acdCfmHistResultPktLossSampleIndex,
        acdCfmHistResultPktLossStatus,
        acdCfmHistResultPktLossDuration,
        acdCfmHistResultPktLossIntervalEnd,
        acdCfmHistResultPktLossSamples,
        acdCfmHistResultPktLossOverflowSamples,
        acdCfmHistResultPktLossHCSamples,
        acdCfmHistResultPktLossNbrLoss,
        acdCfmHistResultPktLossOverflowNbrLoss,
        acdCfmHistResultPktLossHCNbrLoss,
        acdCfmHistResultPktLossNbrGaps,
        acdCfmHistResultPktLossOverflowNbrGaps,
        acdCfmHistResultPktLossHCNbrGaps,
        acdCfmHistResultPktLossLargestGap,
        acdCfmHistResultPktLossOverflowLargestGap,
        acdCfmHistResultPktLossHCLargestGap,
        acdCfmHistResultPktLossRatio,
        acdCfmHistResultPktLossName
    }
    STATUS      current
    DESCRIPTION
       "Objects for Packet loss history result Group."
    ::= { acdCfmGroups 12 }

acdCfmMepStatsTxGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepStatsTxCcmPdu,
        acdCfmMepStatsTxLbmPdu,
        acdCfmMepStatsTxLbrPdu,
        acdCfmMepStatsTxLtmPdu,
        acdCfmMepStatsTxLtrPdu,
        acdCfmMepStatsTxAisPdu,
        acdCfmMepStatsTxLckPdu,
        acdCfmMepStatsTxTstPdu,
        acdCfmMepStatsTxLinearApsPdu,
        acdCfmMepStatsTxRingApsPdu,
        acdCfmMepStatsTxMccPdu,
        acdCfmMepStatsTxLmmPdu,
        acdCfmMepStatsTxLmrPdu,
        acdCfmMepStatsTx1dmPdu,
        acdCfmMepStatsTxDmmPdu,
        acdCfmMepStatsTxDmrPdu,
        acdCfmMepStatsTxExmPdu,
        acdCfmMepStatsTxExrPdu,
        acdCfmMepStatsTxVsmPdu,
        acdCfmMepStatsTxVsrPdu,
        acdCfmMepStatsTxCsfPdu,
        acdCfmMepStatsTxSlmPdu,
        acdCfmMepStatsTxSlrPdu,
        acdCfmMepStatsTxName
    }
    STATUS      current
    DESCRIPTION
       "Objects for MEP transmit statistics Group."
    ::= { acdCfmGroups 13 }

acdCfmMepStatsRxGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepStatsRxCcmPdu,
        acdCfmMepStatsRxLbmPdu,
        acdCfmMepStatsRxLbrPdu,
        acdCfmMepStatsRxLtmPdu,
        acdCfmMepStatsRxLtrPdu,
        acdCfmMepStatsRxAisPdu,
        acdCfmMepStatsRxLckPdu,
        acdCfmMepStatsRxTstPdu,
        acdCfmMepStatsRxLinearApsPdu,
        acdCfmMepStatsRxRingApsPdu,
        acdCfmMepStatsRxMccPdu,
        acdCfmMepStatsRxLmmPdu,
        acdCfmMepStatsRxLmrPdu,
        acdCfmMepStatsRx1dmPdu,
        acdCfmMepStatsRxDmmPdu,
        acdCfmMepStatsRxDmrPdu,
        acdCfmMepStatsRxExmPdu,
        acdCfmMepStatsRxExrPdu,
        acdCfmMepStatsRxVsmPdu,
        acdCfmMepStatsRxVsrPdu,
        acdCfmMepStatsRxCcmSeqErrors,
        acdCfmMepStatsRxLtrUnexpectedPdu,
        acdCfmMepStatsRxLtrMacErrors,
        acdCfmMepStatsRxLbrOooErrors,
        acdCfmMepStatsRxLbrUnexpectedPdu,
        acdCfmMepStatsRxLbrDataErrors,
        acdCfmMepStatsRxCsfPdu,
        acdCfmMepStatsRxSlrPdu,
        acdCfmMepStatsRxCsfInvalidFlags,
        acdCfmMepStatsRxName
    }
    STATUS      current
    DESCRIPTION
       "Objects for MEP receive statistics Group."
    ::= { acdCfmGroups 14 }

acdCfmMepDmStatsGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepDmStatsTxDmmPdu,
        acdCfmMepDmStatsRxDmmPdu,
        acdCfmMepDmStatsTxDmrPdu,
        acdCfmMepDmStatsRxDmrPdu,
        acdCfmMepDmStatsName
    }
    STATUS      current
    DESCRIPTION
       "Objects for DMM/DMR MEP statistics Group."
    ::= { acdCfmGroups 15 }

acdCfmMepStackGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepIdx
    }
    STATUS      current
    DESCRIPTION
       "Objects for cfm Stack Group."
    ::= { acdCfmGroups 16 }

acdCfmMepSlmStatsGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepStatsTxSlmPdu,
        acdCfmMepStatsRxSlmPdu,
        acdCfmMepStatsTxSlrPdu,
        acdCfmMepStatsRxSlrPdu
    }
    STATUS      current
    DESCRIPTION
       "Objects for SLM/SLR MEP statistics Group."
    ::= { acdCfmGroups 17 }

acdCfmSlmCfgGroup OBJECT-GROUP
    OBJECTS {
        acdCfmSlmCfgRowStatus,
        acdCfmSlmCfgMepIdx,
        acdCfmSlmCfgRemoteMepId,
        acdCfmSlmCfgPriority,
        acdCfmSlmCfgState,
        acdCfmSlmCfgInterval,
        acdCfmSlmCfgRefPeriod,
        acdCfmSlmCfgNearEndThresh,
        acdCfmSlmCfgFarEndThresh,
        acdCfmSlmCfgName
    }
    STATUS      current
    DESCRIPTION
       "Objects for SLM configuration Group."
    ::= { acdCfmGroups 18 }

acdCfmSlmResultGroup OBJECT-GROUP
    OBJECTS {
        acdCfmSlmResultPeriodIndex,
        acdCfmSlmResultIntervalStart,
        acdCfmSlmResultValid,
        acdCfmSlmResultNearEndAlert,
        acdCfmSlmResultFarEndAlert,
        acdCfmSlmResultTxSlm,
        acdCfmSlmResultRxSlr,
        acdCfmSlmResultRemoteRxSlm,
        acdCfmSlmResultNearEndNbrLoss,
        acdCfmSlmResultFarEndNbrLoss,
        acdCfmSlmResultNearEndRatio,
        acdCfmSlmResultFarEndRatio,
        acdCfmSlmResultNbrGaps,
        acdCfmSlmResultLargestGap,
        acdCfmSlmResultName
    }
    STATUS      current
    DESCRIPTION
       "Objects for SLM result Group."
    ::= { acdCfmGroups 19 }

acdCfmSlmHistResultGroup OBJECT-GROUP
    OBJECTS {
	acdCfmSlmHistResultID,
	acdCfmSlmHistResultPeriodIndex,
	acdCfmSlmHistResultIntervalEnd,
	acdCfmSlmHistResultTxSlm,
	acdCfmSlmHistResultRxSlr,
	acdCfmSlmHistResultRemoteRxSlm,
	acdCfmSlmHistResultNearEndRatio,
	acdCfmSlmHistResultFarEndRatio,
	acdCfmSlmHistResultNbrGaps,
	acdCfmSlmHistResultLargestGap,
	acdCfmSlmHistResultInstanceIndex,
	acdCfmSlmHistResultName
    }
    STATUS      current
    DESCRIPTION
       "Objects for SLM history result Group."
    ::= { acdCfmGroups 20 }

acdCfmMepCfgGroup OBJECT-GROUP
    OBJECTS {
        acdCfmMepCfgRowStatus,
        acdCfmMepCfgMdIdx,
        acdCfmMepCfgMaIdx,
        acdCfmMepCfgMepId,
        acdCfmMepCfgName,
        acdCfmMepCfgPortId,
        acdCfmMepCfgPortIdMacAddr,
        acdCfmMepCfgDirection,
        acdCfmMepCfgPrimaryVid,
        acdCfmMepCfgActive,
        acdCfmMepCfgCciEnable,
        acdCfmMepCfgCcmSeqEnable,
        acdCfmMepCfgPriority,
        acdCfmMepCfgAlarmPri,
        acdCfmMepCfgFngAlarmTime,
        acdCfmMepCfgFngResetTime,
        acdCfmMepCfgFpEnable,
        acdCfmMepCfgFpPortId,
        acdCfmMepCfgCsfEnable,
        acdCfmMepCfgInterfaceStatusTLVEnable
    }
    STATUS      current
    DESCRIPTION
       "Objects for MEP Config Group."
    ::= { acdCfmGroups 21 }

acdCfmCfgIfAssignGroup OBJECT-GROUP
    OBJECTS {
        acdCfmCfgIfAssignRowStatus,
        acdCfmCfgIfAssignIfName,
        acdCfmCfgIfAssignLockAssign
    }
    STATUS      current
    DESCRIPTION
       "Objects for configuration of interface assign Group."
    ::= { acdCfmGroups 22 }


acdCfmCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
       "The compliance statement for support of the ACD-CFM-MIB module."
    MODULE
        MANDATORY-GROUPS {
            acdCfmDmCfgGroup,
            acdCfmResultOneWayDelayGroup,
            acdCfmResultOneWayDvGroup,
            acdCfmResultTwoWayDelayGroup,
            acdCfmResultTwoWayDvGroup,
            acdCfmHistResultOneWayDelayGroup,
            acdCfmHistResultOneWayDvGroup,
            acdCfmHistResultTwoWayDelayGroup,
            acdCfmHistResultTwoWayDvGroup,
            acdCfmPktLossCfgGroup,
            acdCfmResultPktLossGroup,
            acdCfmHistResultPktLossGroup,
            acdCfmMepStatsTxGroup,
            acdCfmMepStatsRxGroup,
            acdCfmMepDmStatsGroup,
            acdCfmMepStackGroup,
            acdCfmMepSlmStatsGroup,
            acdCfmSlmCfgGroup,
            acdCfmSlmResultGroup,
            acdCfmSlmHistResultGroup,
            acdCfmMepCfgGroup,
            acdCfmCfgIfAssignGroup
         }

    OBJECT  acdCfmDmCfgRowStatus
      SYNTAX       RowStatus { active(1) }
      WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
      DESCRIPTION "Support for createAndWait is not required."

    OBJECT  acdCfmPktLossCfgRowStatus
      SYNTAX       RowStatus { active(1) }
      WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
      DESCRIPTION "Support for createAndWait is not required."

    OBJECT  acdCfmSlmCfgRowStatus
      SYNTAX       RowStatus { active(1) }
      DESCRIPTION "Support for createAndWait is not required."

    OBJECT  acdCfmMepCfgRowStatus
      SYNTAX       RowStatus { active(1) }
      WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
      DESCRIPTION "Support for createAndWait is not required."

    OBJECT  acdCfmCfgIfAssignRowStatus
      SYNTAX       RowStatus { active(1) }
      WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
      DESCRIPTION "Support for createAndWait is not required."


    ::= { acdCfmCompliances 1 }
END

